;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Organic Response ON##OTHER##
DTI TYPE2 CONT 3100LM 1200 WHITE 3K_29480;141;3;3000;2936;Aluminium - Fagerhult - BetaOpti;1365;2936;3000;3000;20;59;157;White;Aluminium - Fagerhult - White;7320046222000;29480;19;19;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 3100LM 1200 WHITE 3K_29470;141;3;3000;2936;Aluminium - Fagerhult - BetaOpti;1365;2936;3000;3000;20;59;157;White;Aluminium - Fagerhult - White;7320046221003;29470;19;19;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 3100LM 1200 WHITE 3K_29470-16;141;3;3000;2936;Aluminium - Fagerhult - BetaOpti;1365;2936;3000;3000;20;59;157;White;Aluminium - Fagerhult - White;7320046221027;29470-16;19;19;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 3100LM 1200 WHITE 3K_29470-402;141;3;3000;2936;Aluminium - Fagerhult - BetaOpti;1365;2936;3000;3000;20;59;147;White;Aluminium - Fagerhult - White;7320046221041;29470-402;20;20;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 3100LM 1200 WHITE 3K_29470-449;141;3;3000;2936;Aluminium - Fagerhult - BetaOpti;1365;2936;3000;3000;20;59;147;White;Aluminium - Fagerhult - White;7320046221089;29470-449;20;20;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 3100LM 1200 WHITE 3K_29470-515;141;3;3000;2936;Aluminium - Fagerhult - BetaOpti;1365;2936;3000;3000;20;59;151;White;Aluminium - Fagerhult - White;7320046688868;29470-515;19;19;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 4800LM 1200 WHITE 3K_29471;141;3;3000;4851;Aluminium - Fagerhult - BetaOpti;1365;4851;3000;3000;20;59;151;White;Aluminium - Fagerhult - White;7320046221102;29471;32;32;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 4800LM 1200 WHITE 3K_29471-402;141;3;3000;4851;Aluminium - Fagerhult - BetaOpti;1365;4851;3000;3000;20;59;147;White;Aluminium - Fagerhult - White;7320046221140;29471-402;33;33;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 4800LM 1200 WHITE 3K_29471-449;141;3;3000;4851;Aluminium - Fagerhult - BetaOpti;1365;4851;3000;3000;20;59;147;White;Aluminium - Fagerhult - White;7320046221188;29471-449;33;33;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 4800LM 1200 WHITE 3K_29471-515;141;3;3000;4851;Aluminium - Fagerhult - BetaOpti;1365;4851;3000;3000;20;59;148;White;Aluminium - Fagerhult - White;7320046688882;29471-515;32;32;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 3K_29472;141;3;3000;5781;Aluminium - Fagerhult - BetaOpti;1365;5781;3000;3000;20;59;158;White;Aluminium - Fagerhult - White;7320046221201;29472;37;37;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 3K_29472-16;141;3;3000;5781;Aluminium - Fagerhult - BetaOpti;1365;5781;3000;3000;20;59;158;White;Aluminium - Fagerhult - White;7320046221225;29472-16;37;37;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 3K_29472-402;141;3;3000;5781;Aluminium - Fagerhult - BetaOpti;1365;5781;3000;3000;20;59;153;White;Aluminium - Fagerhult - White;7320046221249;29472-402;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 3K_29472-449;141;3;3000;5781;Aluminium - Fagerhult - BetaOpti;1365;5781;3000;3000;20;59;153;White;Aluminium - Fagerhult - White;7320046221287;29472-449;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 3K_29472-515;141;3;3000;5781;Aluminium - Fagerhult - BetaOpti;1365;5781;3000;3000;20;82;155;White;Aluminium - Fagerhult - White;7320046688899;29472-515;37;37;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 3K_29472-533;141;3;3000;5781;Aluminium - Fagerhult - BetaOpti;1365;5781;3000;3000;20;82;153;White;Aluminium - Fagerhult - White;7320047806292;29472-533;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;1
DTI TYPE2 6400LM 1200 WHITE 3K_29473;141;3;3000;6519;Aluminium - Fagerhult - BetaOpti;1365;6519;3000;3000;20;59;156;White;Aluminium - Fagerhult - White;7320046221362;29473;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 6400LM 1200 WHITE 3K_29473-402;141;3;3000;6519;Aluminium - Fagerhult - BetaOpti;1365;6519;3000;3000;20;59;156;White;Aluminium - Fagerhult - White;7320046221386;29473-402;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 6400LM 1200 WHITE 3K_29473-449;141;3;3000;6519;Aluminium - Fagerhult - BetaOpti;1365;6519;3000;3000;20;59;156;White;Aluminium - Fagerhult - White;7320046221423;29473-449;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 6400LM 1200 WHITE 3K_29473-474;141;3;3000;6519;Aluminium - Fagerhult - BetaOpti;1365;6519;3000;3000;20;59;150;White;Aluminium - Fagerhult - White;7320046534639;29473-474;43;43;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 6400LM 1200 WHITE 3K_29473-515;141;3;3000;6519;Aluminium - Fagerhult - BetaOpti;1365;6519;3000;3000;20;59;154;White;Aluminium - Fagerhult - White;7320046688912;29473-515;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 6400LM 1200 WHITE 3K_29473-533;141;3;3000;6519;Aluminium - Fagerhult - BetaOpti;1365;6519;3000;3000;20;59;152;White;Aluminium - Fagerhult - White;7320047806315;29473-533;43;43;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 3100LM 1200 WHITE 4K_29474;141;3;4000;3021;Aluminium - Fagerhult - BetaOpti;1365;3021;4000;4000;20;59;162;White;Aluminium - Fagerhult - White;7320046221508;29474;19;19;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 3100LM 1200 WHITE 4K_29474-16;141;3;4000;3021;Aluminium - Fagerhult - BetaOpti;1365;3021;4000;4000;20;59;162;White;Aluminium - Fagerhult - White;7320046221522;29474-16;19;19;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 3100LM 1200 WHITE 4K_29474-402;141;3;4000;3021;Aluminium - Fagerhult - BetaOpti;1365;3021;4000;4000;20;59;151;White;Aluminium - Fagerhult - White;7320046221546;29474-402;20;20;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 3100LM 1200 WHITE 4K_29474-449;141;3;4000;3021;Aluminium - Fagerhult - BetaOpti;1365;3021;4000;4000;20;59;151;White;Aluminium - Fagerhult - White;7320046221584;29474-449;20;20;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 3100LM 1200 WHITE 4K_29474-515;141;3;4000;3021;Aluminium - Fagerhult - BetaOpti;1365;3021;4000;4000;20;59;156;White;Aluminium - Fagerhult - White;7320046688929;29474-515;19;19;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 4800LM 1200 WHITE 4K_29475;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;59;155;White;Aluminium - Fagerhult - White;7320046221607;29475;32;32;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 4800LM 1200 WHITE 4K_29475-16;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;59;155;White;Aluminium - Fagerhult - White;7320046221621;29475-16;32;32;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 4800LM 1200 WHITE 4K_29475-402;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;59;151;White;Aluminium - Fagerhult - White;7320046221645;29475-402;33;33;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 4800LM 1200 WHITE 4K_29475-449;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;59;151;White;Aluminium - Fagerhult - White;7320046221683;29475-449;33;33;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 4800LM 1200 WHITE 4K_29475-515;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;59;152;White;Aluminium - Fagerhult - White;7320046688943;29475-515;32;32;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;1
DTI TYPE2 5600LM 1200 WHITE 4K_29476;141;3;4000;5947;Aluminium - Fagerhult - BetaOpti;1365;5947;4000;4000;20;59;162;White;Aluminium - Fagerhult - White;7320046221706;29476;37;37;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 4K_29476-16;141;3;4000;5947;Aluminium - Fagerhult - BetaOpti;1365;5947;4000;4000;20;59;162;White;Aluminium - Fagerhult - White;7320046221720;29476-16;37;37;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 4K_29476-402;141;3;4000;5947;Aluminium - Fagerhult - BetaOpti;1365;5947;4000;4000;20;59;158;White;Aluminium - Fagerhult - White;7320046221744;29476-402;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 4K_29476-449;141;3;4000;5947;Aluminium - Fagerhult - BetaOpti;1365;5947;4000;4000;20;59;158;White;Aluminium - Fagerhult - White;7320046221782;29476-449;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 4K_29476-515;141;3;4000;5947;Aluminium - Fagerhult - BetaOpti;1365;5947;4000;4000;20;59;159;White;Aluminium - Fagerhult - White;7320046688967;29476-515;37;37;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 4K_29476-533;141;3;4000;5947;Aluminium - Fagerhult - BetaOpti;1365;5947;4000;4000;20;59;157;White;Aluminium - Fagerhult - White;7320047806308;29476-533;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;1
DTI TYPE2 6400LM 1200 WHITE 4K_29477;141;3;4000;6706;Aluminium - Fagerhult - BetaOpti;1365;6706;4000;4000;20;59;161;White;Aluminium - Fagerhult - White;7320046221867;29477;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 6400LM 1200 WHITE 4K_29477-402;141;3;4000;6706;Aluminium - Fagerhult - BetaOpti;1365;6706;4000;4000;20;59;161;White;Aluminium - Fagerhult - White;7320046221881;29477-402;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 6400LM 1200 WHITE 4K_29477-449;141;3;4000;6706;Aluminium - Fagerhult - BetaOpti;1365;6706;4000;4000;20;59;161;White;Aluminium - Fagerhult - White;7320046221928;29477-449;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 6400LM 1200 WHITE 4K_29477-515;141;3;4000;6706;Aluminium - Fagerhult - BetaOpti;1365;6706;4000;4000;20;59;158;White;Aluminium - Fagerhult - White;7320046688974;29477-515;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 6400LM 1200 WHITE 4K_29477-533;141;3;4000;6706;Aluminium - Fagerhult - BetaOpti;1365;6706;4000;4000;20;59;156;White;Aluminium - Fagerhult - White;7320047806322;29477-533;43;43;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;1
DTI TYPE2 CONT 3100LM 1200 WHITE 3K_29480-402;141;3;3000;2936;Aluminium - Fagerhult - BetaOpti;1365;2936;3000;3000;20;59;147;White;Aluminium - Fagerhult - White;7320046222024;29480-402;20;20;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 4800LM 1200 WHITE 3K_29481;141;3;3000;4851;Aluminium - Fagerhult - BetaOpti;1365;4851;3000;3000;20;59;151;White;Aluminium - Fagerhult - White;7320046222048;29481;32;32;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 4800LM 1200 WHITE 3K_29481-402;141;3;3000;4851;Aluminium - Fagerhult - BetaOpti;1365;4851;3000;3000;20;59;147;White;Aluminium - Fagerhult - White;7320046222062;29481-402;33;33;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 5600LM 1200 WHITE 3K_29482;141;3;3000;5781;Aluminium - Fagerhult - BetaOpti;1365;5781;3000;3000;20;59;158;White;Aluminium - Fagerhult - White;7320046222086;29482;37;37;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 5600LM 1200 WHITE 3K_29482-402;141;3;3000;5781;Aluminium - Fagerhult - BetaOpti;1365;5781;3000;3000;20;59;153;White;Aluminium - Fagerhult - White;7320046222109;29482-402;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 6500LM 1200 WHITE 3K_29483;141;3;3000;6519;Aluminium - Fagerhult - BetaOpti;1365;6519;3000;3000;20;59;156;White;Aluminium - Fagerhult - White;7320046222123;29483;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 6500LM 1200 WHITE 3K_29483-402;141;3;3000;6519;Aluminium - Fagerhult - BetaOpti;1365;6519;3000;3000;20;59;156;White;Aluminium - Fagerhult - White;7320046222147;29483-402;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 3100LM 1200 WHITE 4K_29484;141;3;4000;3021;Aluminium - Fagerhult - BetaOpti;1365;3021;4000;4000;20;59;162;White;Aluminium - Fagerhult - White;7320046222161;29484;19;19;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 3100LM 1200 WHITE 4K_29484-402;141;3;4000;3021;Aluminium - Fagerhult - BetaOpti;1365;3021;4000;4000;20;59;151;White;Aluminium - Fagerhult - White;7320046222185;29484-402;20;20;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 4800LM 1200 WHITE 4K_29485;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;59;155;White;Aluminium - Fagerhult - White;7320046222208;29485;32;32;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 4800LM 1200 WHITE 4K_29485-402;141;3;4000;4991;Aluminium - Fagerhult - BetaOpti;1365;4991;4000;4000;20;59;151;White;Aluminium - Fagerhult - White;7320046222222;29485-402;33;33;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 5600LM 1200 WHITE 4K_29486;141;3;4000;5947;Aluminium - Fagerhult - BetaOpti;1365;5947;4000;4000;20;59;162;White;Aluminium - Fagerhult - White;7320046222246;29486;37;37;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 5600LM 1200 WHITE 4K_29486-402;141;3;4000;5947;Aluminium - Fagerhult - BetaOpti;1365;5947;4000;4000;20;59;158;White;Aluminium - Fagerhult - White;7320046222260;29486-402;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 6500LM 1200 WHITE 4K_29487;141;3;4000;6706;Aluminium - Fagerhult - BetaOpti;1365;6706;4000;4000;20;59;161;White;Aluminium - Fagerhult - White;7320046222284;29487;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 CONT 6500LM 1200 WHITE 4K_29487-402;141;3;4000;6706;Aluminium - Fagerhult - BetaOpti;1365;6706;4000;4000;20;59;161;White;Aluminium - Fagerhult - White;7320046222307;29487-402;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE TW PLUS_29489;141;3;4000;5657;Aluminium - Fagerhult - BetaOpti;1365;5657;4000;4000;20;59;120;White;Aluminium - Fagerhult - White;7320048104632;29489;47;47;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 90;D;1;0
DTI TYPE2 5600LM 1200 WHITE 3K PLUS_29491-535;141;3.2;3000;5781;Aluminium - Fagerhult - BetaOpti;1365;5781;3000;3000;20;59;151;White;Aluminium - Fagerhult - White;7320047625961;29491-535;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 4K PLUS_29493-535;141;3.2;4000;5947;Aluminium - Fagerhult - BetaOpti;1365;5947;4000;4000;20;59;155;White;Aluminium - Fagerhult - White;7320047625978;29493-535;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 7600LM 30/70 1200 WHITE 3K PLUS_29496-402;141;3.2;3000;7283;Aluminium - Fagerhult - BetaOpti;1365;7283;3000;3000;20;59;141;White;Aluminium - Fagerhult - White;7320047377679;29496-402;52;52;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 7600LM 30/70 1200 WHITE 3K PLUS_29496-474;141;3.2;3000;7283;Aluminium - Fagerhult - BetaOpti;1365;7283;3000;3000;20;59;141;White;Aluminium - Fagerhult - White;7320047377716;29496-474;52;52;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 7600LM 30/70 1200 WHITE 3K PLUS_29496-531;141;3.2;3000;7283;Aluminium - Fagerhult - BetaOpti;1365;7283;3000;3000;20;59;140;White;Aluminium - Fagerhult - White;7320047377730;29496-531;52;52;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 7600LM 30/70 1200 WHITE 4K PLUS_29497-402;141;3.2;4000;7493;Aluminium - Fagerhult - BetaOpti;1365;7493;4000;4000;20;59;145;White;Aluminium - Fagerhult - White;7320047377754;29497-402;52;52;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 7600LM 30/70 1200 WHITE 4K PLUS_29497-474;141;3.2;4000;7493;Aluminium - Fagerhult - BetaOpti;1365;7493;4000;4000;20;59;145;White;Aluminium - Fagerhult - White;7320047377792;29497-474;52;52;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 7600LM 30/70 1200 WHITE 4K PLUS_29497-531;141;3.2;4000;7493;Aluminium - Fagerhult - BetaOpti;1365;7493;4000;4000;20;59;144;White;Aluminium - Fagerhult - White;7320047377815;29497-531;52;52;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1500 WHITE 4K_29668;141;3.2;4000;5970;Aluminium - Fagerhult - BetaOpti;1665;5970;4000;4000;20;59;162;White;Aluminium - Fagerhult - White;7320046415761;29668;37;37;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1500 WHITE 4K_29668-402;141;3.2;4000;5970;Aluminium - Fagerhult - BetaOpti;1665;5970;4000;4000;20;59;157;White;Aluminium - Fagerhult - White;7320046600822;29668-402;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1500 WHITE 4K_29668-449;141;3.2;4000;5970;Aluminium - Fagerhult - BetaOpti;1665;5970;4000;4000;20;59;157;White;Aluminium - Fagerhult - White;7320046415792;29668-449;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 6000LM 1500 WHITE 3K_29670;141;3.2;3000;5803;Aluminium - Fagerhult - BetaOpti;1665;5803;3000;3000;20;59;157;White;Aluminium - Fagerhult - White;7320046600433;29670;37;37;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 6000LM 1500 WHITE 3K_29670-402;141;3.2;3000;5803;Aluminium - Fagerhult - BetaOpti;1665;5803;3000;3000;20;59;152;White;Aluminium - Fagerhult - White;7320046600457;29670-402;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 6000LM 1500 WHITE 3K_29670-449;141;3.2;3000;5803;Aluminium - Fagerhult - BetaOpti;1665;5803;3000;3000;20;59;152;White;Aluminium - Fagerhult - White;7320046600815;29670-449;38;38;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 7500LM 1500 WHITE 3K_29671;141;3.2;3000;7489;Aluminium - Fagerhult - BetaOpti;1665;7489;3000;3000;20;59;156;White;Aluminium - Fagerhult - White;7320046600839;29671;48;48;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 7500LM 1500 WHITE 3K_29671-402;141;3.2;3000;7489;Aluminium - Fagerhult - BetaOpti;1665;7489;3000;3000;20;59;153;White;Aluminium - Fagerhult - White;7320046600877;29671-402;49;49;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 7500LM 1500 WHITE 4K_29672;141;3.2;4000;7705;Aluminium - Fagerhult - BetaOpti;1665;7705;4000;4000;20;59;161;White;Aluminium - Fagerhult - White;7320046600891;29672;48;48;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 7500LM 1500 WHITE 4K_29672-402;141;3.2;4000;7705;Aluminium - Fagerhult - BetaOpti;1665;7705;4000;4000;20;59;157;White;Aluminium - Fagerhult - White;7320046600907;29672-402;49;49;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 4800LM 1200 WHITE 3K_29471-16;141;3;3000;4851;Aluminium - Fagerhult - BetaOpti;1365;4851;3000;3000;20;59;151;White;Aluminium - Fagerhult - White;7320046221126;29471-16;32;32;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;0
DTI TYPE2 5600LM 1200 WHITE 3K PLUS_29491-546;141;3.4;3000;5781;Aluminium - Fagerhult - BetaOpti;1365;5781;3000;3000;20;58;150;White;Aluminium - Fagerhult - White;7320048521767;29491-546;39;39;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;1
DTI TYPE2 5600LM 1200 WHITE 4K PLUS_29493-546;141;3.4;4000;5947;Aluminium - Fagerhult - BetaOpti;1365;5947;4000;4000;20;58;154;White;Aluminium - Fagerhult - White;7320048521774;29493-546;39;39;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;1
DTI TYPE2 6400LM 1200 WHITE 3K PLUS_29478-533;141;3;3000;6519;Aluminium - Fagerhult - BetaOpti;1365;6519;3000;3000;20;59;152;White;Aluminium - Fagerhult - White;7320047941214;29478-533;43;43;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;1
DTI TYPE2 6400LM 1200 WHITE 4K PLUS_29479-533;141;3;4000;6706;Aluminium - Fagerhult - BetaOpti;1365;6706;4000;4000;20;59;156;White;Aluminium - Fagerhult - White;7320047941269;29479-533;43;43;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;1
DTI TYPE2 7500LM 1500 WHITE 4K_29672-533;141;3.2;4000;7505;Aluminium - Fagerhult - BetaOpti;1665;7505;4000;4000;20;59;157;White;Aluminium - Fagerhult - White;7320049989153;29672-533;49;49;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;1
DTI TYPE2 5600LM 1200 WHITE 3K PLUS_29491-570;141;3.3;3000;5781;Aluminium - Fagerhult - BetaOpti;1365;5781;3000;3000;20;59;136;White;Aluminium - Fagerhult - White;7316912144064;29491-570;42;42;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;1
DTI TYPE2 4800LM 1200 WHITE 3K_29471-570;141;3;3000;4851;Aluminium - Fagerhult - BetaOpti;1365;4851;3000;3000;20;59;138;White;Aluminium - Fagerhult - White;7316912144095;29471-570;35;35;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;1
DTI TYPE2 3100LM 1200 WHITE 3K_29470-570;141;3;3000;2936;Aluminium - Fagerhult - BetaOpti;1365;2936;3000;3000;20;59;137;White;Aluminium - Fagerhult - White;7316912144071;29470-570;21;21;DTI LED Type 2;Wire suspension via friction locks on the luminaire. Wire suspension ordered separately, see Accessories.;A suspended workplace luminaire that produces direct/indirect light. Beta Opti louvres with direct light provide high efficiency and optimal lighting comfort.;min. 80;C;1;1
