;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
RECESSO BETA OPTI 600X600 3900LM 3K 4C_25789;597;3.7;3000;4333;Aluminium - Fagerhult - Beta Opti;597;4333;3000;3000;20;71;141;White;Steel - Fagerhult - White;7320046218256;25789;31;31;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 3K 4C_25789-3;597;3.7;3000;4333;Aluminium - Fagerhult - Beta Opti;597;4333;3000;3000;20;71;141;White;Steel - Fagerhult - White;7320046218294;25789-3;31;31;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 3K 4C_25789-111;597;3.7;3000;4333;Aluminium - Fagerhult - Beta Opti;597;4333;3000;3000;20;71;141;White;Steel - Fagerhult - White;7320046218270;25789-111;31;31;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 3K 4C_25789-340;597;3.7;3000;4333;Aluminium - Fagerhult - Beta Opti;597;4333;3000;3000;20;71;141;White;Steel - Fagerhult - White;7320046218317;25789-340;31;31;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 3K 4C_25789-402;597;3.7;3000;3950;Aluminium - Fagerhult - Beta Opti;597;3950;3000;3000;20;71;135;White;Steel - Fagerhult - White;7320046218331;25789-402;30;30;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 3K 4C_25789-454;597;3.7;3000;3950;Aluminium - Fagerhult - Beta Opti;597;3950;3000;3000;20;71;135;White;Steel - Fagerhult - White;7320046218355;25789-454;30;30;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 3K 4C_25789-456;597;3.7;3000;3950;Aluminium - Fagerhult - Beta Opti;597;3950;3000;3000;20;71;135;White;Steel - Fagerhult - White;7320046218379;25789-456;30;30;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 3K 4C_25789-533;597;3.700;3000;3950;Aluminium - Fagerhult - Beta Opti;597;3950;3000;3000;20;71;134;White;Steel - Fagerhult - White;7320047815034;25789-533;30.1;30.1;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 4K 4C_25791;597;3.7;4000;4343;Aluminium - Fagerhult - Beta Opti;597;4343;4000;4000;20;71;145;White;Steel - Fagerhult - White;7320046218393;25791;30;30;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 4K 4C_25791-3;597;3.7;4000;4343;Aluminium - Fagerhult - Beta Opti;597;4343;4000;4000;20;71;145;White;Steel - Fagerhult - White;7320046218430;25791-3;30;30;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 4K 4C_25791-111;597;3.7;4000;4343;Aluminium - Fagerhult - Beta Opti;597;4343;4000;4000;20;71;145;White;Steel - Fagerhult - White;7320046218416;25791-111;30;30;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 4K 4C_25791-340;597;3.7;4000;4343;Aluminium - Fagerhult - Beta Opti;597;4343;4000;4000;20;71;145;White;Steel - Fagerhult - White;7320046218454;25791-340;30;30;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 4K 4C_25791-402;597;3.7;4000;3950;Aluminium - Fagerhult - Beta Opti;597;3950;4000;4000;20;71;144;White;Steel - Fagerhult - White;7320046218478;25791-402;29;29;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 4K 4C_25791-454;597;3.7;4000;3950;Aluminium - Fagerhult - Beta Opti;597;3950;4000;4000;20;71;144;White;Steel - Fagerhult - White;7320046218492;25791-454;29;29;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 4K 4C_25791-456;597;3.7;4000;3950;Aluminium - Fagerhult - Beta Opti;597;3950;4000;4000;20;71;144;White;Steel - Fagerhult - White;7320046218515;25791-456;29;29;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 3900LM 4K 4C_25791-533;597;3.700;4000;3950;Aluminium - Fagerhult - Beta Opti;597;3950;4000;4000;20;71;141;White;Steel - Fagerhult - White;7320047815058;25791-533;29.4;29.4;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 3K 4C_25817;597;3.7;3000;5431;Aluminium - Fagerhult - Beta Opti;597;5431;3000;3000;20;71;139;White;Steel - Fagerhult - White;7320046216658;25817;39;39;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 3K 4C_25817-3;597;3.7;3000;5431;Aluminium - Fagerhult - Beta Opti;597;5431;3000;3000;20;71;139;White;Steel - Fagerhult - White;7320046216696;25817-3;39;39;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 3K 4C_25817-111;597;3.7;3000;5431;Aluminium - Fagerhult - Beta Opti;597;5431;3000;3000;20;71;139;White;Steel - Fagerhult - White;7320046216672;25817-111;39;39;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 3K 4C_25817-340;597;3.7;3000;5431;Aluminium - Fagerhult - Beta Opti;597;5431;3000;3000;20;71;139;White;Steel - Fagerhult - White;7320046216719;25817-340;39;39;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 3K 4C_25817-402;597;3.7;3000;5000;Aluminium - Fagerhult - Beta Opti;597;5000;3000;3000;20;71;136;White;Steel - Fagerhult - White;7320046216733;25817-402;38;38;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 3K 4C_25817-454;597;3.7;3000;5000;Aluminium - Fagerhult - Beta Opti;597;5000;3000;3000;20;71;136;White;Steel - Fagerhult - White;7320046216757;25817-454;38;38;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 3K 4C_25817-456;597;3.7;3000;5000;Aluminium - Fagerhult - Beta Opti;597;5000;3000;3000;20;71;136;White;Steel - Fagerhult - White;7320046216771;25817-456;38;38;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 3K 4C_25817-533;597;3.700;3000;5000;Aluminium - Fagerhult - Beta Opti;597;5000;3000;3000;20;71;132;White;Steel - Fagerhult - White;7320047815027;25817-533;39.8;39.8;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 4K 4C_25818;597;3.7;4000;5401;Aluminium - Fagerhult - Beta Opti;597;5401;4000;4000;20;71;143;White;Steel - Fagerhult - White;7320046216795;25818;38;38;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 4K 4C_25818-3;597;3.7;4000;5401;Aluminium - Fagerhult - Beta Opti;597;5401;4000;4000;20;71;143;White;Steel - Fagerhult - White;7320046216832;25818-3;38;38;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 4K 4C_25818-111;597;3.700;4000;5401;Aluminium - Fagerhult - Beta Opti;597;5401;4000;4000;20;71;143;White;Steel - Fagerhult - White;7320046216818;25818-111;38;38;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 4K 4C_25818-340;597;3.7;4000;5401;Aluminium - Fagerhult - Beta Opti;597;5401;4000;4000;20;71;143;White;Steel - Fagerhult - White;7320046216856;25818-340;38;38;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 4K 4C_25818-402;597;3.7;4000;5000;Aluminium - Fagerhult - Beta Opti;597;5000;4000;4000;20;71;143;White;Steel - Fagerhult - White;7320046216870;25818-402;36;36;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 4K 4C_25818-454;597;3.7;4000;5000;Aluminium - Fagerhult - Beta Opti;597;5000;4000;4000;20;71;143;White;Steel - Fagerhult - White;7320046216894;25818-454;36;36;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 4K 4C_25818-456;597;3.7;4000;5000;Aluminium - Fagerhult - Beta Opti;597;5000;4000;4000;20;71;143;White;Steel - Fagerhult - White;7320046216917;25818-456;36;36;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 5500LM 4K 4C_25818-533;597;3.700;4000;5000;Aluminium - Fagerhult - Beta Opti;597;5000;4000;4000;20;71;139;White;Steel - Fagerhult - White;7320047815041;25818-533;37.9;37.9;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 VTB MAX LM 3K 4C_25823-402;597;3.8;3000;9643;Aluminium - Fagerhult - Beta Opti;597;9643;3000;3000;20;71;155;White;Steel - Fagerhult - White;7320049718791;25823-402;66.5;66.5;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;C;2
RECESSO BETA OPTI 600X600 VTB MAX LM 4K 4C_25824-402;597;3.8;4000;10162;Aluminium - Fagerhult - Beta Opti;597;10162;4000;4000;20;71;161;White;Steel - Fagerhult - White;7320049718807;25824-402;66.5;66.5;Recesso Beta Opti;Recessed mounting in suspended ceilings. Only for suspended ceilings with visible T-bars (15 or 25 mm).;0;min. 80;B;2