;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Luminaire##OTHER##
HERO SPA 12KLM WIDE HTG FROSTED 840 WHITE_31610-402;307;7.3;4000;11465;498;11465;4000;4000;65;87;143;White;Aluminium - Fagerhult - White;7320047788871;31610-402;84;84;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;1
HERO SPA 16KLM WIDE HTG FROSTED 840 WHITE_31611-402;307;7.3;4000;15232;498;15232;4000;4000;65;87;146;White;Aluminium - Fagerhult - White;7320047788895;31611-402;109.5;109.5;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;4
HERO SPA 20KLM WIDE HTG FROSTED 840 WHITE_31612-402;307;7.3;4000;18737;498;18737;4000;4000;65;87;143;White;Aluminium - Fagerhult - White;7320047788901;31612-402;137;137;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;4
HERO SPA 12KLM WIDE HTG FROSTED 830 WHITE_31613-402;307;7.3;3000;11465;498;11465;3000;3000;65;87;132;White;Aluminium - Fagerhult - White;7320047788918;31613-402;91;91;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;1
HERO SPA 16KLM WIDE HTG FROSTED 830 WHITE_31614-402;307;7.3;3000;15232;498;15232;3000;3000;65;87;135;White;Aluminium - Fagerhult - White;7320047788925;31614-402;118;118;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;4
HERO SPA 20KLM WIDE HTG FROSTED 830 WHITE_31615-402;307;7.3;3000;18737;498;18737;3000;3000;65;87;132;White;Aluminium - Fagerhult - White;7320047788932;31615-402;148.5;148.5;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;4
HERO SPA 12KLM WIDE HTG 840 WHITE_31620-402;307;7.3;4000;12068;498;12068;4000;4000;65;87;157;White;Aluminium - Fagerhult - White;7320047310058;31620-402;80.5;80.5;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;2
HERO SPA 16KLM WIDE HTG 840 WHITE_31621-402;307;7.3;4000;16034;498;16034;4000;4000;65;87;162;White;Aluminium - Fagerhult - White;7320047310072;31621-402;104;104;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;3
HERO SPA 20KLM WIDE HTG 840 WHITE_31622-402;307;7.3;4000;19723;498;19723;4000;4000;65;87;154;White;Aluminium - Fagerhult - White;7320047310089;31622-402;135;135;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;3
HERO SPA 12KLM ASYM. HTG 840 WHITE_31623-402;307;7.3;4000;12497;498;12497;4000;4000;65;87;167;White;Aluminium - Fagerhult - White;7320047310102;31623-402;78.5;78.5;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;5
HERO SPA 16KLM ASYM. HTG 840 WHITE_31624-402;307;7.3;4000;16027;498;16027;4000;4000;65;87;163;White;Aluminium - Fagerhult - White;7320047310119;31624-402;102.5;102.5;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;5
HERO SPA 12KLM WIDE HTG 830 WHITE_31625-402;307;7.3;3000;12068;498;12068;3000;3000;65;87;146;White;Aluminium - Fagerhult - White;7320047310164;31625-402;86.5;86.5;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;2
HERO SPA 16KLM WIDE HTG 830 WHITE_31626-402;307;7.3;3000;16034;498;16034;3000;3000;65;87;150;White;Aluminium - Fagerhult - White;7320047310171;31626-402;112;112;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;3
HERO SPA 20KLM WIDE HTG 830 WHITE_31627-402;307;7.3;3000;19723;498;19723;3000;3000;65;87;142;White;Aluminium - Fagerhult - White;7320047310195;31627-402;145.5;145.5;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;3
HERO SPA 12KLM ASYM. HTG 830 WHITE_31628-402;307;7.3;3000;12497;498;12497;3000;3000;65;87;155;White;Aluminium - Fagerhult - White;7320047310201;31628-402;84.5;84.5;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;5
HERO SPA 16KLM ASYM. HTG 830 WHITE_31629-402;307;7.3;3000;16027;498;16027;3000;3000;65;87;152;White;Aluminium - Fagerhult - White;7320047310218;31629-402;111;111;Hero SPA;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Specially designed for swimming pools. Asymmetrical version for placement at the side of the pool for simpler installation and service. Glare-free with various lumen packages and a good, glare-free light even from higher heights.;min. 80;E;1;5
