;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Length##LENGTH##MILLIMETERS;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##
Notor 65 Indirect Start/Single 1200 3000K DaliPhasePulseControl Anodised_13500-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13500-402.IES;Notor 65 Indirect;aluminium;2750;Fagerhult_Delta _microprisma;Pendant;Pendant;1256;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;2750;3000;3000;20;65;120;Created 20/06/2017;DaliPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046642099;Notor 65 Indirect Start/Single;13500-402;23;min. 80
Notor 65 Indirect Start/Single 1200 4000K DaliPhasePulseControl Anodised_13501-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13501-402.IES;Notor 65 Indirect;aluminium;2900;Fagerhult_Delta _microprisma;Pendant;Pendant;1256;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;2900;4000;4000;20;65;126;Created 20/06/2017;DaliPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046642136;Notor 65 Indirect Start/Single;13501-402;23;min. 80
Notor 65 Indirect Start/Single 1200 3000K DaliPhasePulseControl White_13502-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13502-402.IES;Notor 65 Indirect;aluminium;2750;Fagerhult_Delta _microprisma;Pendant;Pendant;1256;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;2750;3000;3000;20;65;120;Created 20/06/2017;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7320046642174;Notor 65 Indirect Start/Single;13502-402;23;min. 80
Notor 65 Indirect Start/Single 1200 4000K DaliPhasePulseControl White_13503-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13503-402.IES;Notor 65 Indirect;aluminium;2900;Fagerhult_Delta _microprisma;Pendant;Pendant;1256;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;2900;4000;4000;20;65;126;Created 20/06/2017;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7320046642211;Notor 65 Indirect Start/Single;13503-402;23;min. 80
Notor 65 Indirect Start/Single 2400 3000K DaliPhasePulseControl Anodised_13504-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13504-402.IES;Notor 65 Indirect;aluminium;5500;Fagerhult_Delta _microprisma;Pendant;Pendant;2505;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;5500;3000;3000;20;65;120;Created 20/06/2017;DaliPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046642259;Notor 65 Indirect Start/Single;13504-402;46;min. 80
Notor 65 Indirect Start/Single 2400 4000K DaliPhasePulseControl Anodised_13505-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13505-402.IES;Notor 65 Indirect;aluminium;5800;Fagerhult_Delta _microprisma;Pendant;Pendant;2505;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;5800;4000;4000;20;65;126;Created 20/06/2017;DaliPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046642297;Notor 65 Indirect Start/Single;13505-402;46;min. 80
Notor 65 Indirect Start/Single 2400 3000K DaliPhasePulseControl White_13506-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13506-402.IES;Notor 65 Indirect;aluminium;5500;Fagerhult_Delta _microprisma;Pendant;Pendant;2505;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;5500;3000;3000;20;65;120;Created 20/06/2017;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7320046642334;Notor 65 Indirect Start/Single;13506-402;46;min. 80
Notor 65 Indirect Start/Single 2400 4000K DaliPhasePulseControl White_13507-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13507-402.IES;Notor 65 Indirect;aluminium;5800;Fagerhult_Delta _microprisma;Pendant;Pendant;2505;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;5800;4000;4000;20;65;126;Created 20/06/2017;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7320046642372;Notor 65 Indirect Start/Single;13507-402;46;min. 80
Notor 65 Indirect Continuous 1200 3000K DaliPhasePulseControl Anodised_13508-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13508-402.IES;Notor 65 Indirect;aluminium;2750;Fagerhult_Delta _microprisma;Pendant;Pendant;1250;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;2750;3000;3000;20;65;120;Created 20/06/2017;DaliPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046642419;Notor 65 Indirect Continuous;13508-402;23;min. 80
Notor 65 Indirect Continuous 1200 4000K DaliPhasePulseControl Anodised_13509-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13509-402.IES;Notor 65 Indirect;aluminium;2900;Fagerhult_Delta _microprisma;Pendant;Pendant;1250;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;2900;4000;4000;20;65;126;Created 20/06/2017;DaliPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046642457;Notor 65 Indirect Continuous;13509-402;23;min. 80
Notor 65 Indirect Continuous 1200 3000K DaliPhasePulseControl White_13510-402;65;3.0;3000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13510-402.IES;Notor 65 Indirect;aluminium;2750;Fagerhult_Delta _microprisma;Pendant;Pendant;1250;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;2750;3000;3000;20;65;120;Created 20/06/2017;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7320046642495;Notor 65 Indirect Continuous;13510-402;23;min. 80
Notor 65 Indirect Continuous 1200 4000K DaliPhasePulseControl White_13511-402;65;3.0;4000;L 1200 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13511-402.IES;Notor 65 Indirect;aluminium;2900;Fagerhult_Delta _microprisma;Pendant;Pendant;1250;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;2900;4000;4000;20;65;126;Created 20/06/2017;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7320046642532;Notor 65 Indirect Continuous;13511-402;23;min. 80
Notor 65 Indirect Continuous 2400 3000K DaliPhasePulseControl Anodised_13512-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13512-402.IES;Notor 65 Indirect;aluminium;5500;Fagerhult_Delta _microprisma;Pendant;Pendant;2499;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;5500;3000;3000;20;65;120;Created 20/06/2017;DaliPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046642570;Notor 65 Indirect Continuous;13512-402;46;min. 80
Notor 65 Indirect Continuous 2400 4000K DaliPhasePulseControl Anodised_13513-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13513-402.IES;Notor 65 Indirect;aluminium;5800;Fagerhult_Delta _microprisma;Pendant;Pendant;2499;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;5800;4000;4000;20;65;126;Created 20/06/2017;DaliPhasePulseControl;Anodised;Fagerhult_Alugrey_Aluminium;7320046642617;Notor 65 Indirect Continuous;13513-402;46;min. 80
Notor 65 Indirect Continuous 2400 3000K DaliPhasePulseControl White_13514-402;65;6.0;3000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13514-402.IES;Notor 65 Indirect;aluminium;5500;Fagerhult_Delta _microprisma;Pendant;Pendant;2499;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;5500;3000;3000;20;65;120;Created 20/06/2017;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7320046642655;Notor 65 Indirect Continuous;13514-402;46;min. 80
Notor 65 Indirect Continuous 2400 4000K DaliPhasePulseControl White_13515-402;65;6.0;4000;L 2400 mm + W 65 mm + H 65 mm;Rectangle;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;13515-402.IES;Notor 65 Indirect;aluminium;5800;Fagerhult_Delta _microprisma;Pendant;Pendant;2499;Luminaire body enameled in white (RAL 9016) or natural anodised, extruded aluminium finish.;5800;4000;4000;20;65;126;Created 20/06/2017;DaliPhasePulseControl;White;Fagerhult_White_aluminium;7320046642693;Notor 65 Indirect Continuous;13515-402;46;min. 80
