;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Installation##OTHER##;Type Continuous##OTHER##;Type Start Single##OTHER##
NOTOR65 SURF/PEND 30/70 1200 LL DELTA 840_13660-20027;65;3;4000;5883;Acrylic - Fagerhult - Delta Microprism;1256;5883;4000;4000;20;65;150;White;Aluminium - Fagerhult - White;7320049863507;13660-20027;41;41;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;1;0;2
NOTOR65 SURF/PEND 30/70 1700 LL DELTA 840_13660-20032;65;4;4000;7979;Acrylic - Fagerhult - Delta Microprism;1673;7979;4000;4000;20;65;144;White;Aluminium - Fagerhult - White;7320049863651;13660-20032;57.5;57.5;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;1;0;3
NOTOR65 SURF/PEND D 800 LL DELTA 840_13660-20047;65;2.1;4000;1033;Acrylic - Fagerhult - Delta Microprism;840;1033;4000;4000;20;65;117;White;Aluminium - Fagerhult - White;7320049874701;13660-20047;9.5;9.5;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;1;0;1
NOTOR65 SURF/PEND 50/50 1200 LL DELTA 840_13660-20049;65;3.6;4000;3050;Acrylic - Fagerhult - Delta Microprism;1256;3050;4000;4000;20;65;139;White;Aluminium - Fagerhult - White;7320049874763;13660-20049;23;23;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;1;0;2
NOTOR65 SURF/PEND D 1200 LL DELTA 840_13660-20048;65;3.5;4000;1550;Acrylic - Fagerhult - Delta Microprism;1256;1550;4000;4000;20;65;136;White;Aluminium - Fagerhult - White;7320049874732;13660-20048;12;12;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;1;0;1
NOTOR65 SURF/PEND D 2400 LL DELTA 840_13660-20050;65;6.4;4000;3100;Acrylic - Fagerhult - Delta Microprism;2506;3100;4000;4000;20;65;136;White;Aluminium - Fagerhult - White;7320049874794;13660-20050;24;24;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;1;0;1
NOTOR65 SURF/PEND 50/50 2400 LL DELTA 840_13660-20051;65;6.5;4000;6100;Acrylic - Fagerhult - Delta Microprism;2506;6100;4000;4000;20;65;139;White;Aluminium - Fagerhult - White;7320049874824;13660-20051;46;46;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;1;0;4
NOTOR65 SURF/PEND 50/50 2400 LL DELTA 840_13660-21003;65;6.4;4000;6100;Acrylic - Fagerhult - Delta Microprism;2502;6100;4000;4000;20;65;139;White;Aluminium - Fagerhult - White;7316911855664;13660-21003;46;46;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;2;4;0
NOTOR65 SURF/PEND D 1200 LL DELTA 840_13660-20927;65;3.5;4000;1550;Acrylic - Fagerhult - Delta Microprism;1256;1550;4000;4000;20;65;136;White;Aluminium - Fagerhult - White;7316911856753;13660-20927;12;12;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;1;0;1
NOTOR65 SURF/PEND D 2400 LL DELTA 840_13660-20955;65;6.4;4000;3100;Acrylic - Fagerhult - Delta Microprism;2506;3100;4000;4000;20;65;136;White;Aluminium - Fagerhult - White;7316911855596;13660-20955;24;24;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;1;0;1
NOTOR65 SURF/PEND D 800 LL DELTA 840_13660-20971;65;2;4000;1033;Acrylic - Fagerhult - Delta Microprism;836;1033;4000;4000;20;65;117;White;Aluminium - Fagerhult - White;7316911855824;13660-20971;9.5;9.5;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;2;1;0
NOTOR65 SURF/PEND D 1200 LL DELTA 840_13660-20979;65;3.4;4000;1550;Acrylic - Fagerhult - Delta Microprism;1252;1550;4000;4000;20;65;136;White;Aluminium - Fagerhult - White;7316911856524;13660-20979;12;12;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;2;1;0
NOTOR65 SURF/PEND D 2400 LL DELTA 840_13660-20995;65;6.3;4000;3100;Acrylic - Fagerhult - Delta Microprism;2502;3100;4000;4000;20;65;136;White;Aluminium - Fagerhult - White;7316911856975;13660-20995;24;24;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;2;1;0
NOTOR65 SURF/PEND 50/50 1200 LL DELTA 840_13660-20944;65;3.6;4000;3050;Acrylic - Fagerhult - Delta Microprism;1256;3050;4000;4000;20;65;139;White;Aluminium - Fagerhult - White;7316911856364;13660-20944;23;23;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;1;0;2
NOTOR65 SURF/PEND 50/50 2400 LL DELTA 840_13660-20963;65;6.5;4000;6100;Acrylic - Fagerhult - Delta Microprism;2506;6100;4000;4000;20;65;139;White;Aluminium - Fagerhult - White;7316911856029;13660-20963;46;46;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;1;0;4
NOTOR65 SURF/PEND 50/50 1200 LL DELTA 840_13660-20987;65;3.5;4000;3050;Acrylic - Fagerhult - Delta Microprism;1252;3050;4000;4000;20;65;139;White;Aluminium - Fagerhult - White;7316911856234;13660-20987;23;23;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;2;2;0
NOTOR65 SURF/PEND D 800 LL DELTA 840_13660-20919;65;2.1;4000;1033;Acrylic - Fagerhult - Delta Microprism;840;1033;4000;4000;20;65;117;White;Aluminium - Fagerhult - White;7316911855893;13660-20919;9.5;9.5;Notor 65 Delta;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Delta louvres provide high efficiency and optimal lighting comfort. Single or continuous installation.;min. 80;C;1;1;0;1
