,Width##LENGTH##MILLIMETERS,Weight (Kg)##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,Voltage Loss##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,URL##OTHER##,Type Comments##OTHER##,Type##OTHER##,Total Light Loss Factor##OTHER##,Tilt Angle##ANGLE##DEGREES,Photometric File Note##OTHER##,Model##OTHER##,Lamp##OTHER##,IP Code##OTHER##,EAN_Code##OTHER##,Control##OTHER##,Color Rendering Index##OTHER##,Color##OTHER##,Body##OTHER##,Temperature Loss##OTHER##,Temperature Color##OTHER##,Sus Position##LENGTH##MILLIMETERS,Sus Height##LENGTH##MILLIMETERS,Surface Depreciation Loss##OTHER##,Photometric Web File##OTHER##,None##OTHER##,Manufacturer##OTHER##,Luminous Intensity##ELECTRICAL_LUMINOUS_INTENSITY##CANDELAS,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Luminaire Dirt Depreciation##OTHER##,Louvre##OTHER##,Load Classification##OTHER##,Light Loss Input Method##OTHER##,Light Loss Factor##OTHER##,Length##LENGTH##MILLIMETERS,Lamp Tilt Loss##OTHER##,Lamp Lumen Depreciation##OTHER##,Initial Light Intensity Input Method##OTHER##,Initial Intensity##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Initial Color##OTHER##,Illuminance##ELECTRICAL_ILLUMINANCE##LUX,Height##LENGTH##MILLIMETERS,End Cap 2##OTHER##,End Cap##OTHER##,Emit from Rectangle Width##LENGTH##MILLIMETERS,Emit from Rectangle Length##LENGTH##MILLIMETERS,Emit Shape Visible in Rendering##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT,Dimming Lamp Color Temperature Shift##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,Color Filter##OTHER##,Ballast Loss##OTHER##,BIM Version##OTHER##,At a distance##LENGTH##MILLIMETERS,Assembly Code##OTHER##,Article Number##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES
NOTOR65 SURF/PEND 50/50 1200 LL BETA 840_ESenseOrganic_13314-533,65.000000000000,2.9,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320047806551,1,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1358.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1352.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13314-533,37.000000000000
NOTOR65 SURF/PEND D 1200 LL BETA 830_DaliPhasePulseControl_13300-402,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046630874,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2138.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13300-402,17.000000000000
NOTOR65 BETAOPTI SURF PEND 1200 D LL 830 ALU START/SINGLE_ESenseActive_13300-442,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046630911,2,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2090.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,109.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13300-442,20.000000000000
NOTOR65 BETAOPTI SURF PEND 1200 D LL 830 ALU START/SINGLE_PhasePulse_13300-449,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046630898,0,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2138.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13300-449,17.000000000000
NOTOR65 SURF/PEND D 1200 HL BETA 830_DaliPhasePulseControl_13301-402,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046630959,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3411.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,131.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13301-402,27.500000000000
NOTOR65 BETAOPTI SURF PEND 1200 D HL 830 ALU START/SINGLE_ESenseActive_13301-442,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046630997,2,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3334.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,115.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13301-442,30.000000000000
NOTOR65 BETAOPTI SURF PEND 1200 D HL 830 ALU START/SINGLE_PhasePulse_13301-449,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046630973,0,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3411.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,131.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13301-449,27.500000000000
NOTOR65 SURF/PEND D 1200 LL BETA 840_DaliPhasePulseControl_13302-402,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631031,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2200.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13302-402,17.000000000000
NOTOR65 BETAOPTI SURF PEND 1200 D LL 840 ALU START/SINGLE_ESenseActive_13302-442,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631079,2,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2200.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,115.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13302-442,20.000000000000
NOTOR65 BETAOPTI SURF PEND 1200 D LL 840 ALU START/SINGLE_PhasePulse_13302-449,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631055,0,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2200.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13302-449,17.000000000000
NOTOR65 SURF/PEND D 1200 HL BETA 840_DaliPhasePulseControl_13303-402,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631116,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3509.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,135.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13303-402,27.500000000000
NOTOR65 BETAOPTI SURF PEND 1200 D HL 840 ALU START/SINGLE_ESenseActive_13303-442,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631154,2,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3509.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,121.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13303-442,30.000000000000
NOTOR65 BETAOPTI SURF PEND 1200 D HL 840 ALU START/SINGLE_PhasePulse_13303-449,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631130,0,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3509.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,135.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13303-449,27.500000000000
NOTOR65 SURF/PEND D 1200 LL BETA 830_DaliPhasePulseControl_13304-402,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631192,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2138.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13304-402,17.000000000000
NOTOR65 BETAOPTI SURF PEND 1200 D LL 830 WHT START/SINGLE_ESenseActive_13304-442,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631239,2,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2090.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,109.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13304-442,20.000000000000
NOTOR65 BETAOPTI SURF PEND 1200 D LL 830 WHT START/SINGLE_PhasePulse_13304-449,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631215,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2138.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13304-449,17.000000000000
NOTOR65 SURF/PEND D 1200 HL BETA 830_DaliPhasePulseControl_13305-402,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631277,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3411.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,131.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13305-402,27.500000000000
NOTOR65 BETAOPTI SURF PEND 1200 D HL 830 WHT START/SINGLE_ESenseActive_13305-442,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631314,2,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3334.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,115.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13305-442,30.000000000000
NOTOR65 BETAOPTI SURF PEND 1200 D HL 830 WHT START/SINGLE_PhasePulse_13305-449,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631291,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3411.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,131.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13305-449,27.500000000000
NOTOR65 SURF/PEND D 1200 LL BETA 840_DaliPhasePulseControl_13306-402,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631352,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2200.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13306-402,17.000000000000
NOTOR65 BETAOPTI SURF PEND 1200 D LL 840 WHT START/SINGLE_ESenseActive_13306-442,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631390,2,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2200.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,115.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13306-442,20.000000000000
NOTOR65 BETAOPTI SURF PEND 1200 D LL 840 WHT START/SINGLE_PhasePulse_13306-449,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631376,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2200.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13306-449,17.000000000000
NOTOR65 SURF/PEND D 1200 HL BETA 840_DaliPhasePulseControl_13307-402,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631437,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3509.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,135.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13307-402,27.500000000000
NOTOR65 BETAOPTI SURF PEND 1200 D HL 840 WHT START/SINGLE_ESenseActive_13307-442,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631475,2,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3509.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,121.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13307-442,30.000000000000
NOTOR65 BETAOPTI SURF PEND 1200 D HL 840 WHT START/SINGLE_PhasePulse_13307-449,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631451,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3509.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,135.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13307-449,27.500000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 830_DaliPhasePulseControl_13308-402,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631512,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4666.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13308-402,37.000000000000
NOTOR65 BETAOPTI PEND 1200 DI LL 830 ALU START/SINGLE_ESenseActive_13308-442,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631550,2,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4560.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,124.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13308-442,38.800000000000
NOTOR65 BETAOPTI PEND 1200 DI LL 830 ALU START/SINGLE_PhasePulse_13308-449,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631536,0,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4666.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13308-449,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 830_ESenseOrganic_13308-533,65.000000000000,2.9,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320047806520,1,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4666.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1358.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1352.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13308-533,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 HL BETA 830_DaliPhasePulseControl_13309-402,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631598,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5914.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,137.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13309-402,45.000000000000
NOTOR65 BETAOPTI PEND 1200 DI HL 830 ALU START/SINGLE_ESenseActive_13309-442,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631635,2,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5914.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,137.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13309-442,45.000000000000
NOTOR65 BETAOPTI PEND 1200 DI HL 830 ALU START/SINGLE_PhasePulse_13309-449,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631611,0,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5914.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,137.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13309-449,45.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 840_DaliPhasePulseControl_13310-402,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631673,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13310-402,37.000000000000
NOTOR65 BETAOPTI PEND 1200 DI LL 840 ALU START/SINGLE_ESenseActive_13310-442,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631710,2,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13310-442,38.500000000000
NOTOR65 BETAOPTI PEND 1200 DI LL 840 ALU START/SINGLE_PhasePulse_13310-449,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631697,0,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13310-449,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 840_ESenseOrganic_13310-533,65.000000000000,2.9,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320047806537,1,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1358.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1352.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13310-533,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 HL BETA 840_DaliPhasePulseControl_13311-402,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631758,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6084.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,141.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13311-402,45.000000000000
NOTOR65 BETAOPTI PEND 1200 DI HL 840 ALU START/SINGLE_ESenseActive_13311-442,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631796,2,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6084.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,132.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13311-442,47.500000000000
NOTOR65 BETAOPTI PEND 1200 DI HL 840 ALU START/SINGLE_PhasePulse_13311-449,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631772,0,min. 80,Anodised,Aluminium - Fagerhult - Anodised,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6084.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,141.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13311-449,45.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 830_DaliPhasePulseControl_13312-402,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631833,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4666.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13312-402,37.000000000000
NOTOR65 BETAOPTI PEND 1200 DI LL 830 WHT START/SINGLE_ESenseActive_13312-442,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631871,2,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4560.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,124.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13312-442,38.800000000000
NOTOR65 BETAOPTI PEND 1200 DI LL 830 WHT START/SINGLE_PhasePulse_13312-449,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631857,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4666.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13312-449,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 830_ESenseOrganic_13312-533,65.000000000000,2.9,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320047806544,1,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4666.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1358.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1352.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13312-533,37.000000000000
NOTOR65 BETAOPTI PEND 1200 DI LL 830 WHT START/SINGLE_ESenseActive_13312-539,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320047644023,2,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4666.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13312-539,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 HL BETA 830_DaliPhasePulseControl_13313-402,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631918,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5914.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,137.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13313-402,45.000000000000
NOTOR65 BETAOPTI PEND 1200 DI HL 830 WHT START/SINGLE_ESenseActive_13313-442,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631956,2,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5746.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,125.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13313-442,48.000000000000
NOTOR65 BETAOPTI PEND 1200 DI HL 830 WHT START/SINGLE_PhasePulse_13313-449,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631932,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5914.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,137.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13313-449,45.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 840_DaliPhasePulseControl_13314-402,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046631994,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13314-402,37.000000000000
NOTOR65 BETAOPTI PEND 1200 DI LL 840 WHT START/SINGLE_ESenseActive_13314-442,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632038,2,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13314-442,38.500000000000
NOTOR65 BETAOPTI PEND 1200 DI LL 840 WHT START/SINGLE_PhasePulse_13314-449,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632014,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13314-449,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 HL BETA 840_DaliPhasePulseControl_13315-402,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632076,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6084.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,141.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13315-402,45.000000000000
NOTOR65 BETAOPTI PEND 1200 DI HL 840 WHT START/SINGLE_ESenseActive_13315-442,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632113,2,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6084.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,132.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13315-442,47.500000000000
NOTOR65 BETAOPTI PEND 1200 DI HL 840 WHT START/SINGLE_PhasePulse_13315-449,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632090,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6084.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,141.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13315-449,45.000000000000
NOTOR65 SURF/PEND D 2400 LL BETA 830_DaliPhasePulseControl_13316-402,65.000000000000,5.4,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632151,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4276.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13316-402,35.000000000000
NOTOR65 SURF/PEND D 2400 HL BETA 830_DaliPhasePulseControl_13317-402,65.000000000000,5.4,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632199,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6822.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,132.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13317-402,55.000000000000
NOTOR65 SURF/PEND D 2400 LL BETA 840_DaliPhasePulseControl_13318-402,65.000000000000,5.4,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632236,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4400.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13318-402,35.000000000000
NOTOR65 SURF/PEND D 2400 HL BETA 840_DaliPhasePulseControl_13319-402,65.000000000000,5.4,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632274,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,7018.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,135.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13319-402,55.000000000000
NOTOR65 SURF/PEND D 2400 LL BETA 830_DaliPhasePulseControl_13320-402,65.000000000000,5.4,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632311,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4276.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13320-402,35.000000000000
NOTOR65 SURF/PEND D 2400 HL BETA 830_DaliPhasePulseControl_13321-402,65.000000000000,5.4,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632359,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6822.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,132.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13321-402,55.000000000000
NOTOR65 SURF/PEND D 2400 LL BETA 840_DaliPhasePulseControl_13322-402,65.000000000000,5.4,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632397,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4400.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13322-402,35.000000000000
NOTOR65 SURF/PEND D 2400 HL BETA 840_DaliPhasePulseControl_13323-402,65.000000000000,5.4,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632434,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,7018.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,135.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13323-402,55.000000000000
NOTOR65 SURF/PEND 50/50 2400 LL BETA 830_DaliPhasePulseControl_13324-402,65.000000000000,5.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632472,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,9332.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13324-402,73.000000000000
NOTOR65 SURF/PEND 50/50 2400 HL BETA 830_DaliPhasePulseControl_13325-402,65.000000000000,5.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632519,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,11828.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,137.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13325-402,90.000000000000
NOTOR65 SURF/PEND 50/50 2400 LL BETA 840_DaliPhasePulseControl_13326-402,65.000000000000,5.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632557,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,9600.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13326-402,73.000000000000
NOTOR65 SURF/PEND 50/50 2400 HL BETA 840_DaliPhasePulseControl_13327-402,65.000000000000,5.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632595,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,12168.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,141.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13327-402,90.000000000000
NOTOR65 SURF/PEND 50/50 2400 LL BETA 830_DaliPhasePulseControl_13328-402,65.000000000000,5.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632632,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,9332.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13328-402,73.000000000000
NOTOR65 SURF/PEND 50/50 2400 HL BETA 830_DaliPhasePulseControl_13329-402,65.000000000000,5.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632670,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,11828.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,137.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13329-402,90.000000000000
NOTOR65 SURF/PEND 50/50 2400 LL BETA 840_DaliPhasePulseControl_13330-402,65.000000000000,5.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632717,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,9600.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13330-402,73.000000000000
NOTOR65 SURF/PEND 50/50 2400 HL BETA 840_DaliPhasePulseControl_13331-402,65.000000000000,5.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632755,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,12168.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,141.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13331-402,90.000000000000
NOTOR65 SURF/PEND D 1200 LL BETA 830_DaliPhasePulseControl_13332-402,65.000000000000,2.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632793,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2138.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13332-402,17.000000000000
NOTOR65 SURF/PEND D 1200 HL BETA 830_DaliPhasePulseControl_13333-402,65.000000000000,2.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632830,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3411.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,131.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13333-402,27.500000000000
NOTOR65 SURF/PEND D 1200 LL BETA 840_DaliPhasePulseControl_13334-402,65.000000000000,2.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632878,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2200.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13334-402,18.000000000000
NOTOR65 SURF/PEND D 1200 HL BETA 840_DaliPhasePulseControl_13335-402,65.000000000000,2.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632915,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3509.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,135.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13335-402,27.500000000000
NOTOR65 SURF/PEND D 1200 LL BETA 830_DaliPhasePulseControl_13336-402,65.000000000000,2.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632953,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2138.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13336-402,17.000000000000
NOTOR65 SURF/PEND D 1200 HL BETA 830_DaliPhasePulseControl_13337-402,65.000000000000,2.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046632991,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3411.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,131.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13337-402,27.500000000000
NOTOR65 SURF/PEND D 1200 LL BETA 840_DaliPhasePulseControl_13338-402,65.000000000000,2.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633035,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2200.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13338-402,18.000000000000
NOTOR65 SURF/PEND D 1200 HL BETA 840_DaliPhasePulseControl_13339-402,65.000000000000,2.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633073,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,3509.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,135.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13339-402,27.500000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 830_DaliPhasePulseControl_13340-402,65.000000000000,2.7,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633110,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4666.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13340-402,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 HL BETA 830_DaliPhasePulseControl_13341-402,65.000000000000,2.7,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633158,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5914.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,137.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13341-402,48.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 840_DaliPhasePulseControl_13342-402,65.000000000000,2.7,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633196,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13342-402,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 HL BETA 840_DaliPhasePulseControl_13343-402,65.000000000000,2.7,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633233,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6084.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,141.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13343-402,45.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 830_DaliPhasePulseControl_13344-402,65.000000000000,2.7,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633271,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4666.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13344-402,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 HL BETA 830_DaliPhasePulseControl_13345-402,65.000000000000,2.7,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633318,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5914.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,137.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13345-402,48.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 840_DaliPhasePulseControl_13346-402,65.000000000000,2.7,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633356,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13346-402,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 HL BETA 840_DaliPhasePulseControl_13347-402,65.000000000000,2.7,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633394,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6084.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1261.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1255.000000000000,0,141.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13347-402,45.000000000000
NOTOR65 SURF/PEND D 2400 LL BETA 830_DaliPhasePulseControl_13348-402,65.000000000000,5.3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633431,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4276.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13348-402,35.000000000000
NOTOR65 SURF/PEND D 2400 HL BETA 830_DaliPhasePulseControl_13349-402,65.000000000000,5.3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633479,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6822.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,132.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13349-402,55.000000000000
NOTOR65 SURF/PEND D 2400 LL BETA 840_DaliPhasePulseControl_13350-402,65.000000000000,5.3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046633516,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4400.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13350-402,35.000000000000
NOTOR65 SURF/PEND D 2400 HL BETA 840_DaliPhasePulseControl_13351-402,65.000000000000,5.3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635282,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,7018.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,135.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13351-402,55.000000000000
NOTOR65 SURF/PEND D 2400 LL BETA 830_DaliPhasePulseControl_13352-402,65.000000000000,5.3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635329,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4276.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13352-402,35.000000000000
NOTOR65 SURF/PEND D 2400 HL BETA 830_DaliPhasePulseControl_13353-402,65.000000000000,5.3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635367,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6822.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,132.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13353-402,55.000000000000
NOTOR65 SURF/PEND D 2400 LL BETA 840_DaliPhasePulseControl_13354-402,65.000000000000,5.3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635404,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4400.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13354-402,35.000000000000
NOTOR65 SURF/PEND D 2400 HL BETA 840_DaliPhasePulseControl_13355-402,65.000000000000,5.3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635442,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,7018.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,135.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13355-402,55.000000000000
NOTOR65 SURF/PEND 50/50 2400 LL BETA 830_DaliPhasePulseControl_13356-402,65.000000000000,5.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635480,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,9332.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13356-402,73.000000000000
NOTOR65 SURF/PEND 50/50 2400 HL BETA 830_DaliPhasePulseControl_13357-402,65.000000000000,5.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635527,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,11828.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,137.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13357-402,90.000000000000
NOTOR65 SURF/PEND 50/50 2400 LL BETA 840_DaliPhasePulseControl_13358-402,65.000000000000,5.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635565,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,9600.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13358-402,73.000000000000
NOTOR65 SURF/PEND 50/50 2400 HL BETA 840_DaliPhasePulseControl_13359-402,65.000000000000,5.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635602,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,12168.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,141.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13359-402,90.000000000000
NOTOR65 SURF/PEND 50/50 2400 LL BETA 830_DaliPhasePulseControl_13360-402,65.000000000000,5.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635640,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,9332.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13360-402,73.000000000000
NOTOR65 SURF/PEND 50/50 2400 HL BETA 830_DaliPhasePulseControl_13361-402,65.000000000000,5.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635688,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,11828.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13361-402,90.000000000000
NOTOR65 SURF/PEND 50/50 2400 LL BETA 840_DaliPhasePulseControl_13362-402,65.000000000000,5.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635725,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,9600.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13362-402,73.000000000000
NOTOR65 SURF/PEND 50/50 2400 HL BETA 840_DaliPhasePulseControl_13363-402,65.000000000000,5.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320046635763,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,12168.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2522.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2516.000000000000,0,141.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13363-402,90.000000000000
NOTOR65 BETAOPTI PEND 1200 DI HL 830 WHT START/SINGLE_ESenseOrganic_13313-546,65.000000000000,3.1,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320048521781,1,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5914.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1427.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1421.000000000000,0,132.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13313-546,47.000000000000
NOTOR65 BETAOPTI PEND 1200 DI HL 840 WHT START/SINGLE_ESenseOrganic_13315-546,65.000000000000,3.1,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320048521927,1,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6084.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1427.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1421.000000000000,0,136.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13315-546,47.000000000000
NOTOR65 SURF/PEND 50/50 1200 HL BETA 830_PhasePulse_13309-554,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049595705,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5914.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,137.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13309-554,45.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 830_PhasePulse_13308-554,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049595682,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4666.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13308-554,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 HL BETA 840_PhasePulse_13311-554,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049595743,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6084.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,141.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13311-554,45.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 840_PhasePulse_13310-554,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049595729,0,min. 80,Alugrey,Aluminium - Fagerhult - Alugrey,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13310-554,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 830_PhasePulse_13312-554,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049595767,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4666.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13312-554,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 HL BETA 830_PhasePulse_13313-554,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049595781,0,min. 80,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5914.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,137.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13313-554,45.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 840_PhasePulse_13314-554,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049595804,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13314-554,37.000000000000
NOTOR65 SURF/PEND 50/50 1200 HL BETA 840_PhasePulse_13315-554,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049595828,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6084.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,141.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13315-554,45.000000000000
NOTOR65 SURF/PEND 30/70 1200 LL BETA 840_ESenseActive_13660-20012,65.000000000000,3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049709430,2,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6568.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1357.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1351.000000000000,0,128.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13660-20012,53.500000000000
NOTOR65 SURF/PEND 30/70 1200 LL BETA 840_DaliPhasePulseControl_13660-20013,65.000000000000,2.5,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049709461,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6568.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,128.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13660-20013,53.500000000000
NOTOR65 SURF/PEND 50/50 1200 BETA T/W_DaliPhasePulseControl_13660-20025,65.000000000000,3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049863446,0,min. 90,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5619.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,104.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13660-20025,55.000000000000
NOTOR65 SURF/PEND 50/50 1200 BETA T/W_ESenseOrganic_13660-20026,65.000000000000,3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049863477,1,min. 90,White,Aluminium - Fagerhult - White,1,3000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,5619.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1357.000000000000,1,1,0,,3000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1351.000000000000,0,103.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13660-20026,56.000000000000
NOTOR65 SURF/PEND 30/70 1200 LL BETA 840_ESenseOrganic_13660-20037,65.000000000000,3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049863774,1,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6568.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1357.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1351.000000000000,0,127.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13660-20037,54.500000000000
NOTOR65 SURF/PEND 30/70 1200 LL BETA 840_PhasePulse_13660-20038,65.000000000000,3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049863804,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6568.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,128.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13660-20038,53.500000000000
NOTOR65 SURF/PEND 30/70 1200 LL BETA 840_ESenseActive_13660-20039,65.000000000000,3,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049863835,2,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,6568.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1328.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1322.000000000000,0,128.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13660-20039,53.500000000000
NOTOR65 SURF/PEND D 1200 LL BETA 840_DaliPhasePulseControl_13660-20043,65.000000000000,2.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049874596,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,2200.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,115.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13660-20043,20.000000000000
NOTOR65 SURF/PEND 50/50 1200 LL BETA 840_DaliPhasePulseControl_13660-20044,65.000000000000,2.8,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",1,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049874633,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4800.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,1267.000000000000,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,1261.000000000000,0,138.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13660-20044,37.000000000000
NOTOR65 SURF/PEND D 2400 LL BETA 840_DaliPhasePulseControl_13660-20045,65.000000000000,5.4,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",0,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049874671,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,4400.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,134.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13660-20045,35.000000000000
NOTOR65 SURF/PEND 50/50 2400 LL BETA 840_DaliPhasePulseControl_13660-20046,65.000000000000,5.6,9.290304000000,1,230.000000000000,www.fagerhult.com,"Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.",2,1,-90.000000000000,"The .IES files provided are sample files based on a few standard configurations.  Not all photometric configurations are available.   The actual data and values will vary depending on lens, color temperature and other options.  Please contact manufacturer for more defined photometric data.",Notor 65 Beta Opti,LED,20,7320049876354,0,min. 80,White,Aluminium - Fagerhult - White,1,4000,342.899999999992,1000.000000000000,1,GENERIC - Please download and link the .IES file that best matches your fixture specification,,info@fagerhult.se,109.816910733408,9600.000000000000,1,Aluminium - Fagerhult - BetaOpti,Lighting,0,,2528.000000000001,1,1,0,,4000.000000000000,,11.820593893742,65.000000000000,1,1,59.000000000000,2522.000000000000,0,130.000000000000,0,Suspended or ceiling-mounted workplace luminaire with direct or direct/indirect light. Beta Opti louvres provide high efficiency and optimal lighting comfort. Single or continuous Installation,1219.200000000000,16777215,1,1,3048.000000000000,D5020230,13660-20046,76.500000000000
