;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Zhaga Up##OTHER##;Zhaga Down##OTHER##
CIRRUS G2 STD 3000LM 830_311651-20004;8;3000;3000;PMMA - Fagerhult - Clear;3000;3000;3000;66;259;97;Alu grey;Aluminium - Fagerhult - Alugrey;7316911544803;311651-20004;33;33;578;Cirrus G2;Luminaire for installation on posts with post top Ø 60 mm.;A lamppost that offers Scandinavian contemporary design along with high light comfort from the evenly lit top reflector.;min. 80;E;1;0;0
CIRRUS G2 STD 3000LM 830_311651-20005;8;3000;3000;PMMA - Fagerhult - Clear;3000;3000;3000;66;259;97;Alu grey;Aluminium - Fagerhult - Alugrey;7316911580146;311651-20005;33;33;578;Cirrus G2;Luminaire for installation on posts with post top Ø 60 mm.;A lamppost that offers Scandinavian contemporary design along with high light comfort from the evenly lit top reflector.;min. 80;E;1;0;0
CIRRUS G2 ZHAGA 3000LM 830_311651-20006;8.1;3000;3000;PMMA - Fagerhult - Clear;3000;3000;3000;66;276;92;Alu grey;Aluminium - Fagerhult - Alugrey;7316911580023;311651-20006;34;34;578;Cirrus G2;Luminaire for installation on posts with post top Ø 60 mm.;A lamppost that offers Scandinavian contemporary design along with high light comfort from the evenly lit top reflector.;min. 80;E;1;1;0
CIRRUS G2 ZHAGA 3000LM 830_311651-20007;8.1;3000;3000;PMMA - Fagerhult - Clear;3000;3000;3000;66;276;92;Alu grey;Aluminium - Fagerhult - Alugrey;7316911580061;311651-20007;34;34;578;Cirrus G2;Luminaire for installation on posts with post top Ø 60 mm.;A lamppost that offers Scandinavian contemporary design along with high light comfort from the evenly lit top reflector.;min. 80;E;1;1;0
CIRRUS G2 STD 3000LM 830_311651-20008;8.3;3000;3000;PMMA - Fagerhult - Clear;3000;3000;3000;66;259;92;Alu grey;Aluminium - Fagerhult - Alugrey;7316911580108;311651-20008;34;34;578;Cirrus G2;Luminaire for installation on posts with post top Ø 60 mm.;A lamppost that offers Scandinavian contemporary design along with high light comfort from the evenly lit top reflector.;min. 80;E;1;0;0
CIRRUS G2 STD 3000LM 830_311651-20009;8.3;3000;3000;PMMA - Fagerhult - Clear;3000;3000;3000;66;259;92;Alu grey;Aluminium - Fagerhult - Alugrey;7316911579980;311651-20009;34;34;578;Cirrus G2;Luminaire for installation on posts with post top Ø 60 mm.;A lamppost that offers Scandinavian contemporary design along with high light comfort from the evenly lit top reflector.;min. 80;E;1;0;0
CIRRUS G2 ZHAGA 3000LM 830_311651-20012;8.2;3000;3000;PMMA - Fagerhult - Clear;3000;3000;3000;66;276;92;Alu grey;Aluminium - Fagerhult - Alugrey;7316911618016;311651-20012;34;34;578;Cirrus G2;Luminaire for installation on posts with post top Ø 60 mm.;A lamppost that offers Scandinavian contemporary design along with high light comfort from the evenly lit top reflector.;min. 80;E;1;1;1
CIRRUS G2 ZHAGA 3000LM 830_311651-20013;8.2;3000;3000;PMMA - Fagerhult - Clear;3000;3000;3000;66;276;92;Alu grey;Aluminium - Fagerhult - Alugrey;7316911657879;311651-20013;34;34;578;Cirrus G2;Luminaire for installation on posts with post top Ø 60 mm.;A lamppost that offers Scandinavian contemporary design along with high light comfort from the evenly lit top reflector.;min. 80;E;1;1;1
