;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Twin##OTHER##;Zhaga##OTHER##
RONDO G3 SINGLE POST TOP ASYM DALI HL 830_302270-20002;6.1;3000;3983;Light - Fagerhult - Lens;357;65;291;110;Grey;Aluminium - Fagerhult - Grey;7316910408410;302270-20002;38;Rondo G3 post top;Luminaire for assembly on a post, with post top Ø 60 mm.;A single or dual-configuration lamp post, symmetrical or asymmetric light distribution. An effective, minimalist solution for retail sites, schoolyards and parks. CLO as standard for stable luminous flux over the working life of the luminaire. Zhaga connection as option.;min. 80;E;1;0;0
RONDO G3 SINGLE POST TOP SYM DALI HL 830_302270-20001;6.1;3000;4002;Light - Fagerhult - Lens;357;65;291;112;Grey;Aluminium - Fagerhult - Grey;7316910408373;302270-20001;38;Rondo G3 post top;Luminaire for assembly on a post, with post top Ø 60 mm.;A single or dual-configuration lamp post, symmetrical or asymmetric light distribution. An effective, minimalist solution for retail sites, schoolyards and parks. CLO as standard for stable luminous flux over the working life of the luminaire. Zhaga connection as option.;min. 80;E;1;0;0
RONDO G3 TWIN POST TOP SYM DALI HL 830_302270-20003;11.8;3000;8004;Light - Fagerhult - Lens;714;65;291;112;Grey;Aluminium - Fagerhult - Grey;7316910408434;302270-20003;76;Rondo G3 post top;Luminaire for assembly on a post, with post top Ø 60 mm.;A single or dual-configuration lamp post, symmetrical or asymmetric light distribution. An effective, minimalist solution for retail sites, schoolyards and parks. CLO as standard for stable luminous flux over the working life of the luminaire. Zhaga connection as option.;min. 80;E;1;1;0
