";Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Size##OTHER##"
"GLOBIA CLASSIC TRACK D300/115 LL 830 GLASS GLOBE_59150-20006;2.9;3000;2754;Glass - Fagerhult - Opal;2754;3000;3000;20;450;140;Black;Steel sheet - Fagerhult - Black;7316911148087;59150-20006;20.5;20.5;300;Globia Classic;Two-point suspension c.t.c 70 mm or track assembly in Control track.;A round beam decorative luminaire in three sizes for entrances and stairwells, for example.;min. 80;C;1;1"
"GLOBIA CLASSIC TRACK D400/150 LL 840 GLASS GLOBE_59150-20011;5;4000;3208;Glass - Fagerhult - Opal;3208;4000;4000;20;550;151;White;Steel sheet - Fagerhult - White;7316911150080;59150-20011;22;22;400;Globia Classic;Two-point suspension c.t.c 70 mm or track assembly in Control track.;A round beam decorative luminaire in three sizes for entrances and stairwells, for example.;min. 80;C;1;2"
"GLOBIA CLASSIC TRACK D300/115 LL 840 ACRYLIC GLOBE_59150-20035;2.4;4000;2754;Acrylic - Fagerhult - Opal;2754;4000;4000;20;450;140;Black;Steel sheet - Fagerhult - Black;7316911831422;59150-20035;20.5;20.5;300;Globia Classic;Two-point suspension c.t.c 70 mm or track assembly in Control track.;A round beam decorative luminaire in three sizes for entrances and stairwells, for example.;min. 80;C;1;1"
"GLOBIA CLASSIC TRACK D450/170 LL 840 ACRYLIC GLOBE_59150-20033;4.8;4000;3226;Acrylic - Fagerhult - Opal;3226;4000;4000;20;600;117;White;Steel sheet - Fagerhult - White;7316911831446;59150-20033;28;28;450;Globia Classic;Two-point suspension c.t.c 70 mm or track assembly in Control track.;A round beam decorative luminaire in three sizes for entrances and stairwells, for example.;min. 80;C;1;3"
