;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Luminaire design##OTHER##
OPALUME D/I HALF SPHERE 400 STD 1500LM E1 740_306200-22841;10.3;4000;1741;1741;4000;4000;66;350;95;Grey;Aluminium - Fagerhult - Grey;7316911013965;306200-22841;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM E3 740_306200-22843;10.3;4000;1641;1641;4000;4000;66;350;88;Grey;Aluminium - Fagerhult - Grey;7316911014085;306200-22843;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM E2 740_306200-22842;10.3;4000;1741;1741;4000;4000;66;350;94;Grey;Aluminium - Fagerhult - Grey;7316911014023;306200-22842;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM E5 740_306200-22844;10.3;4000;1741;1741;4000;4000;66;350;94;Grey;Aluminium - Fagerhult - Grey;7316911014146;306200-22844;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM E6 740_306200-22845;10.3;4000;1641;1641;4000;4000;66;350;88;Grey;Aluminium - Fagerhult - Grey;7316911014207;306200-22845;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1600LM E9 740_306200-22846;10.3;4000;1841;1841;4000;4000;66;350;98;Grey;Aluminium - Fagerhult - Grey;7316911014269;306200-22846;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM L2 740_306200-22847;10.3;4000;1741;1741;4000;4000;66;350;95;Grey;Aluminium - Fagerhult - Grey;7316911014320;306200-22847;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM L4 740_306200-22848;10.3;4000;1741;1741;4000;4000;66;350;95;Grey;Aluminium - Fagerhult - Grey;7316911014382;306200-22848;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1400LM L5 740_306200-22850;10.3;4000;1641;1641;4000;4000;66;350;88;Grey;Aluminium - Fagerhult - Grey;7316911014450;306200-22850;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM L7 740_306200-22851;10.3;4000;1741;1741;4000;4000;66;350;95;Grey;Aluminium - Fagerhult - Grey;7316911014511;306200-22851;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM L8 740_306200-22852;10.3;4000;1741;1741;4000;4000;66;350;93;Grey;Aluminium - Fagerhult - Grey;7316911014573;306200-22852;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1400LM F60 740_306200-22853;10.3;4000;1641;1641;4000;4000;66;350;88;Grey;Aluminium - Fagerhult - Grey;7316911014641;306200-22853;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 400 STD 1500LM L9 740_306200-22918;10.3;4000;1741;1741;4000;4000;66;350;93;Grey;Aluminium - Fagerhult - Grey;7316911019455;306200-22918;16;16;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 500 STD 17600LM E1 740_306200-22928;19.3;4000;17866;17866;4000;4000;66;350;144;Grey;Aluminium - Fagerhult - Grey;7316911021175;306200-22928;123;123;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17100LM E2 740_306200-22929;19.3;4000;17366;17366;4000;4000;66;350;140;Grey;Aluminium - Fagerhult - Grey;7316911021267;306200-22929;123;123;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 16200LM E3 740_306200-22930;19.3;4000;16466;16466;4000;4000;66;350;133;Grey;Aluminium - Fagerhult - Grey;7316911021328;306200-22930;122;122;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17500LM E5 740_306200-22931;19.3;4000;17766;17766;4000;4000;66;350;143;Grey;Aluminium - Fagerhult - Grey;7316911021380;306200-22931;123;123;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 16100LM E6 740_306200-22932;19.3;4000;16366;16366;4000;4000;66;350;132;Grey;Aluminium - Fagerhult - Grey;7316911021458;306200-22932;122;122;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17300LM E9 740_306200-22933;19.3;4000;17566;17566;4000;4000;66;350;141;Grey;Aluminium - Fagerhult - Grey;7316911021519;306200-22933;123;123;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17500LM L4 740_306200-22935;19.3;4000;17766;17766;4000;4000;66;350;143;Grey;Aluminium - Fagerhult - Grey;7316911021632;306200-22935;122;122;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17600LM L2 740_306200-22934;19.3;4000;17866;17866;4000;4000;66;350;144;Grey;Aluminium - Fagerhult - Grey;7316911021571;306200-22934;122;122;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 16200LM L5 740_306200-22936;19.3;4000;16466;16466;4000;4000;66;350;132;Grey;Aluminium - Fagerhult - Grey;7316911021700;306200-22936;123;123;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17500LM L7 740_306200-22937;19.3;4000;17766;17766;4000;4000;66;350;143;Grey;Aluminium - Fagerhult - Grey;7316911021762;306200-22937;122;122;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17100LM L8 740_306200-22938;19.3;4000;17366;17366;4000;4000;66;350;140;Grey;Aluminium - Fagerhult - Grey;7316911021823;306200-22938;122;122;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 17100LM L9 740_306200-22939;19.3;4000;17366;17366;4000;4000;66;350;140;Grey;Aluminium - Fagerhult - Grey;7316911021885;306200-22939;123;123;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 500 STD 16300LM F60 740_306200-22940;19.3;4000;16566;16566;4000;4000;66;350;133;Grey;Aluminium - Fagerhult - Grey;7316911021953;306200-22940;123;123;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
OPALUME D/I HALF SPHERE 400 STD 1500LM L11 740_306200-24771;10.3;4000;1741;1741;4000;4000;66;350;91;Grey;Aluminium - Fagerhult - Grey;7316912478275;306200-24771;17;17;400;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;2
OPALUME D/I HALF SPHERE 500 STD 16900LM L11 740_306200-24787;19.3;4000;17166;17166;4000;4000;66;350;139;Grey;Aluminium - Fagerhult - Grey;7316912492585;306200-24787;122;122;507;Opalume Post;Luminaire for mounting on arm, Ø48 mm and Ø60 mm. For mounting top of the post or wall via wall bracket, see Accessories;Post luminaire with high performance and light comfort and CLO for an even output. Available in two different designs, conical and spherical, with the possibility of RGBW. Optimised light pattern with AGC lenses developed for road lighting.;min. 70;D;1;3
