;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
PLEIAD G4 165 REC DALI BLACK WIDE HL 830_73038-402;0.5;3000;2055;Aluminium - Fagerhult - Black;2055;3000;3000;64;98;124;White/Black;Aluminium - Fagerhult - White;7320047818967;73038-402;17;17;183;Pleiad G4 165;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles. Also available with Tunable White, RGB/W and integrated emergency lighting.;min. 80;E;1
PLEIAD G4 165 REC DALI BLACK WIDE HL 840_73040-402;0.5;4000;2105;Aluminium - Fagerhult - Black;2105;4000;4000;64;98;127;White/Black;Aluminium - Fagerhult - White;7320047819322;73040-402;17;17;183;Pleiad G4 165;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles. Also available with Tunable White, RGB/W and integrated emergency lighting.;min. 80;E;1
PLEIAD G4 165 REC DALI MATT WIDE HL 830_73057-402;0.5;3000;2629;Aluminium - Fagerhult - Alugrey;2629;3000;3000;64;98;158;White/alu;Aluminium - Fagerhult - White;7320047820403;73057-402;17;17;183;Pleiad G4 165;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles. Also available with Tunable White, RGB/W and integrated emergency lighting.;min. 80;E;1
PLEIAD G4 165 REC DALI MATT WIDE HL 840_73059-402;0.5;4000;2693;Aluminium - Fagerhult - Alugrey;2693;4000;4000;64;98;162;White/alu;Aluminium - Fagerhult - White;7320047820762;73059-402;17;17;183;Pleiad G4 165;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles. Also available with Tunable White, RGB/W and integrated emergency lighting.;min. 80;E;1
PLEIAD G4 165 REC DALI WHITE WIDE HL 830_73075-402;0.5;3000;2526;Aluminium - Fagerhult - White;2526;3000;3000;64;98;152;White;Aluminium - Fagerhult - White;7320047834165;73075-402;17;17;183;Pleiad G4 165;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles. Also available with Tunable White, RGB/W and integrated emergency lighting.;min. 80;E;1
PLEIAD G4 165 REC DALI WHITE WIDE HL 840_73077-402;0.5;4000;2588;Aluminium - Fagerhult - White;2588;4000;4000;64;98;156;White;Aluminium - Fagerhult - White;7320047834523;73077-402;17;17;183;Pleiad G4 165;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles. Also available with Tunable White, RGB/W and integrated emergency lighting.;min. 80;E;1
