;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
PLEIAD G4 FLEX REC DALI BLACK NARROW HL 830_73200-402;0.4;3000;1136;Aluminium - Fagerhult - Black;1136;3000;3000;20;110;96;White/Black;Aluminium - Fagerhult - White;7320047870071;73200-402;12;12;122;Pleiad G4 Flex;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;A small downlight with very excellent technical lighting properties. Two different luminous fluxes with high colour reproduction. Rotatable 355º and tilts 45º.;min. 80;E;1
PLEIAD G4 FLEX REC DALI BLACK NARROW HL 840_73201-402;0.4;4000;1185;Aluminium - Fagerhult - Black;1185;4000;4000;20;110;100;White/Black;Aluminium - Fagerhult - White;7320047870132;73201-402;12;12;122;Pleiad G4 Flex;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;A small downlight with very excellent technical lighting properties. Two different luminous fluxes with high colour reproduction. Rotatable 355º and tilts 45º.;min. 80;E;1
PLEIAD G4 FLEX REC DALI BLACK MEDIUM HL 830_73204-402;0.4;3000;1290;Aluminium - Fagerhult - Black;1290;3000;3000;20;110;109;White/Black;Aluminium - Fagerhult - White;7320047870316;73204-402;12;12;122;Pleiad G4 Flex;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;A small downlight with very excellent technical lighting properties. Two different luminous fluxes with high colour reproduction. Rotatable 355º and tilts 45º.;min. 80;E;1
PLEIAD G4 FLEX REC DALI BLACK MEDIUM HL 840_73205-402;0.4;4000;1345;Aluminium - Fagerhult - Black;1345;4000;4000;20;110;114;White/Black;Aluminium - Fagerhult - White;7320047870378;73205-402;12;12;122;Pleiad G4 Flex;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;A small downlight with very excellent technical lighting properties. Two different luminous fluxes with high colour reproduction. Rotatable 355º and tilts 45º.;min. 80;E;1
