;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
PLEIAD G4 WW REC DALI SPEC HL 830_73190-402;0.6;3000;2054;2054;3000;3000;20;138;115;White/alu;Aluminium - Fagerhult - White;7320047828942;73190-402;18;18;183;Pleiad G4 Wallwasher;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, , see accessories. For detailed information, see the installation instructions.;An efficient, asymmetrical downlight for illuminating walls with a light that reaches all the way up to the corner of the ceiling. With several luminous fluxes and reflector options, G4 Wallwasher is also available with Tunable White and RGB/W.;min. 80;E;1
PLEIAD G4 WW REC DALI SPEC HL 840_73191-402;0.6;4000;2106;2106;4000;4000;20;138;118;White/alu;Aluminium - Fagerhult - White;7320047829123;73191-402;18;18;183;Pleiad G4 Wallwasher;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, , see accessories. For detailed information, see the installation instructions.;An efficient, asymmetrical downlight for illuminating walls with a light that reaches all the way up to the corner of the ceiling. With several luminous fluxes and reflector options, G4 Wallwasher is also available with Tunable White and RGB/W.;min. 80;E;1
PLEIAD G4 WW REC DALI MATT HL 830_73194-402;0.6;3000;1815;1815;3000;3000;20;138;101;White/alu;Aluminium - Fagerhult - White;7320047829666;73194-402;18;18;183;Pleiad G4 Wallwasher;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, , see accessories. For detailed information, see the installation instructions.;An efficient, asymmetrical downlight for illuminating walls with a light that reaches all the way up to the corner of the ceiling. With several luminous fluxes and reflector options, G4 Wallwasher is also available with Tunable White and RGB/W.;min. 80;E;1
PLEIAD G4 WW REC DALI MATT HL 840_73195-402;0.6;4000;1861;1861;4000;4000;20;138;104;White/alu;Aluminium - Fagerhult - White;7320047829840;73195-402;18;18;183;Pleiad G4 Wallwasher;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, , see accessories. For detailed information, see the installation instructions.;An efficient, asymmetrical downlight for illuminating walls with a light that reaches all the way up to the corner of the ceiling. With several luminous fluxes and reflector options, G4 Wallwasher is also available with Tunable White and RGB/W.;min. 80;E;1
