;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
PLEIAD G4 125 REC DALI MATT WIDE HL 840_73264-402;0.3;4000;2067;Aluminium - Fagerhult - Alugrey;2067;4000;4000;20;98;146;White/alu;Aluminium - Fagerhult - White;7320047838125;73264-402;13;13;143;Pleiad G4 125;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles.;min. 80;D;1
PLEIAD G4 125 REC DALI MATT WIDE HL 830_73262-402;0.3;3000;1971;Aluminium - Fagerhult - Alugrey;1971;3000;3000;20;98;139;White/alu;Aluminium - Fagerhult - White;7320047837760;73262-402;13;13;143;Pleiad G4 125;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles.;min. 80;E;1
PLEIAD G4 125 REC DALI BLACK WIDE HL 840_73256-402;0.3;4000;1847;Aluminium - Fagerhult - Black;1847;4000;4000;20;98;130;White/Black;Aluminium - Fagerhult - White;7320047824180;73256-402;14;14;143;Pleiad G4 125;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles.;min. 80;D;1
PLEIAD G4 125 REC DALI WHITE WIDE HL 840_73272-402;0.3;4000;2030;Aluminium - Fagerhult - White;2030;4000;4000;20;98;143;White;Aluminium - Fagerhult - White;7320047841002;73272-402;13;13;143;Pleiad G4 125;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles.;min. 80;D;1
PLEIAD G4 125 REC DALI BLACK WIDE HL 830_73254-402;0.3;3000;1754;Aluminium - Fagerhult - Black;1754;3000;3000;20;98;124;White/Black;Aluminium - Fagerhult - White;7320047823824;73254-402;14;14;143;Pleiad G4 125;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles.;min. 80;E;1
PLEIAD G4 125 REC DALI WHITE WIDE HL 830_73270-402;0.3;3000;1928;Aluminium - Fagerhult - White;1928;3000;3000;20;98;136;White;Aluminium - Fagerhult - White;7320047840647;73270-402;13;13;143;Pleiad G4 125;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles.;min. 80;D;1
