;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
PLEIAD G4 70 REC DALI MATT MEDIUM HL 830_73231-402;0.3;3000;1097;Aluminium - Fagerhult - Alugrey;1097;3000;3000;44;104;114;White/alu;Aluminium - Fagerhult - White;7320047862465;73231-402;9.6;9.6;82;Pleiad G4 70;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;min. 80;E;1
PLEIAD G4 70 REC DALI WHITE MEDIUM HL 830_73232-402;0.3;3000;1085;Aluminium - Fagerhult - White;1085;3000;3000;44;104;113;White;Aluminium - Fagerhult - White;7320047862526;73232-402;9.6;9.6;82;Pleiad G4 70;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;min. 80;E;1
PLEIAD G4 70 REC DALI BLACK MEDIUM HL 830_73233-402;0.3;3000;921;Aluminium - Fagerhult - Black;921;3000;3000;44;104;96;Black;Aluminium - Fagerhult - Black;7320047862588;73233-402;9.6;9.6;82;Pleiad G4 70;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;min. 80;E;1
PLEIAD G4 70 REC DALI MATT MEDIUM HL 840_73235-402;0.3;4000;1144;Aluminium - Fagerhult - Alugrey;1144;4000;4000;44;104;119;White/alu;Aluminium - Fagerhult - White;7320047862649;73235-402;9.6;9.6;82;Pleiad G4 70;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;min. 80;E;1
PLEIAD G4 70 REC DALI WHITE MEDIUM HL 840_73236-402;0.3;4000;1131;Aluminium - Fagerhult - White;1131;4000;4000;44;104;118;White;Aluminium - Fagerhult - White;7320047862700;73236-402;9.6;9.6;82;Pleiad G4 70;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;min. 80;E;1
PLEIAD G4 70 REC DALI BLACK MEDIUM HL 840_73237-402;0.3;4000;960;Aluminium - Fagerhult - Black;960;4000;4000;44;104;100;Black;Aluminium - Fagerhult - Black;7320047862762;73237-402;9.6;9.6;82;Pleiad G4 70;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;min. 80;E;1
PLEIAD G4 70 REC DALI BLACK MEDIUM HL 830_75201-20711;0.3;3000;921;Aluminium - Fagerhult - Black;921;3000;3000;44;104;96;White/Black;Aluminium - Fagerhult - White;7320048973740;75201-20711;9.6;9.6;82;Pleiad G4 70;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;min. 80;E;1
PLEIAD G4 70 REC DALI BLACK MEDIUM HL 840_75201-20729;0.3;4000;960;Aluminium - Fagerhult - Black;960;4000;4000;44;104;100;White/Black;Aluminium - Fagerhult - White;7316910897481;75201-20729;9.6;9.6;82;Pleiad G4 70;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Recessed mounting in unventilated or ventilated suspended ceilings. Separate ballast and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;min. 80;E;1
