;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
PLEIAD G4 205 REC DALI BLACK WIDE HL 830_73326-402;0.7;3000;2326;Aluminium - Fagerhult - Black;2326;3000;3000;64;106;134;White/Black;Aluminium - Fagerhult - White;7320047845093;73326-402;18;18;223;Pleiad G4 205;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles. Also available with Tunable White, RGB/W and integrated emergency lighting.;min. 80;E;1
PLEIAD G4 205 REC DALI BLACK WIDE HL 840_73328-402;0.7;4000;2272;Aluminium - Fagerhult - Black;2272;4000;4000;64;106;137;White/Black;Aluminium - Fagerhult - White;7320047845451;73328-402;17.5;17.5;223;Pleiad G4 205;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles. Also available with Tunable White, RGB/W and integrated emergency lighting.;min. 80;E;1
PLEIAD G4 205 REC DALI MATT WIDE HL 830_73342-402;0.7;3000;2761;Aluminium - Fagerhult - Alugrey;2761;3000;3000;64;106;159;White/alu;Aluminium - Fagerhult - White;7320047849411;73342-402;18;18;223;Pleiad G4 205;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles. Also available with Tunable White, RGB/W and integrated emergency lighting.;min. 80;E;1
PLEIAD G4 205 REC DALI MATT WIDE HL 840_73344-402;0.7;4000;2697;Aluminium - Fagerhult - Alugrey;2697;4000;4000;64;106;162;White/alu;Aluminium - Fagerhult - White;7320047849770;73344-402;17.5;17.5;223;Pleiad G4 205;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles. Also available with Tunable White, RGB/W and integrated emergency lighting.;min. 80;E;1
PLEIAD G4 205 REC DALI WHITE WIDE HL 830_73358-402;0.7;3000;2693;Aluminium - Fagerhult - White;2693;3000;3000;64;106;155;White;Aluminium - Fagerhult - White;7320047853753;73358-402;18;18;223;Pleiad G4 205;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles. Also available with Tunable White, RGB/W and integrated emergency lighting.;min. 80;E;1
PLEIAD G4 205 REC DALI WHITE WIDE HL 840_73360-402;0.7;4000;2631;Aluminium - Fagerhult - White;2631;4000;4000;64;106;158;White;Aluminium - Fagerhult - White;7320047854118;73360-402;17.5;17.5;223;Pleiad G4 205;Recessed mounting in unventilated or ventilated suspended ceilings. Separate driver and installation clip for easy and tool-free installation supplied as standard. An assembly plate must be used when mounting on soft tile ceilings, see accessories. For detailed information, see the installation instructions.;Efficient downlight with excellent technical lighting properties. Choose between several luminous fluxes, reflector options and distribution angles. Also available with Tunable White, RGB/W and integrated emergency lighting.;min. 80;E;1
