;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;MODEL##OTHER##;Organic Response##OTHER##
DWIDE DELTA REC VTB 300X600 830 WHITE_22194;320;1.8;3000;2020;Acrylic - Fagerhult - Delta Microprism;595;2020;3000;3000;20;57;125;White;Aluminium - Fagerhult - White;7320047636950;22194;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 830 WHITE_22194-3;320;1.8;3000;2020;Acrylic - Fagerhult - Delta Microprism;630;2020;3000;3000;20;57;125;White;Aluminium - Fagerhult - White;7320047636967;22194-3;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 830 WHITE_22194-111;320;1.8;3000;2020;Acrylic - Fagerhult - Delta Microprism;630;2020;3000;3000;20;57;125;White;Aluminium - Fagerhult - White;7320047637001;22194-111;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 830 WHITE_22194-340;320;1.8;3000;2020;Acrylic - Fagerhult - Delta Microprism;630;2020;3000;3000;20;57;125;White;Aluminium - Fagerhult - White;7320047637025;22194-340;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 830 WHITE_22194-402;320;1.8;3000;2183;Acrylic - Fagerhult - Delta Microprism;630;2183;3000;3000;20;57;129;White;Aluminium - Fagerhult - White;7320047636981;22194-402;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 830 WHITE_22194-519;320;1.8;3000;2020;Acrylic - Fagerhult - Delta Microprism;630;2020;3000;3000;20;57;125;White;Aluminium - Fagerhult - White;7320047637063;22194-519;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 830 WHITE_22194-520;320;1.8;3000;2183;Acrylic - Fagerhult - Delta Microprism;630;2183;3000;3000;20;57;129;White;Aluminium - Fagerhult - White;7320047637070;22194-520;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 830 WHITE_22194-528;320;1.8;3000;2183;Acrylic - Fagerhult - Delta Microprism;630;2183;3000;3000;20;57;129;White;Aluminium - Fagerhult - White;7320047637018;22194-528;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 830 WHITE_22194-529;320;1.8;3000;2183;Acrylic - Fagerhult - Delta Microprism;630;2183;3000;3000;20;57;129;White;Aluminium - Fagerhult - White;7320047637032;22194-529;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 840 WHITE_22195;320;1.8;4000;2129;Acrylic - Fagerhult - Delta Microprism;630;2129;4000;4000;20;57;131;White;Aluminium - Fagerhult - White;7320047637087;22195;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 840 WHITE_22195-3;320;1.8;4000;2129;Acrylic - Fagerhult - Delta Microprism;630;2129;4000;4000;20;57;131;White;Aluminium - Fagerhult - White;7320047637094;22195-3;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 840 WHITE_22195-111;320;1.8;4000;2129;Acrylic - Fagerhult - Delta Microprism;630;2129;4000;4000;20;57;131;White;Aluminium - Fagerhult - White;7320047637117;22195-111;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 840 WHITE_22195-340;320;1.8;4000;2129;Acrylic - Fagerhult - Delta Microprism;630;2129;4000;4000;20;57;131;White;Aluminium - Fagerhult - White;7320047637131;22195-340;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 840 WHITE_22195-402;320;1.8;4000;2300;Acrylic - Fagerhult - Delta Microprism;630;2300;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047637100;22195-402;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 840 WHITE_22195-519;320;1.8;4000;2129;Acrylic - Fagerhult - Delta Microprism;630;2129;4000;4000;20;57;131;White;Aluminium - Fagerhult - White;7320047637155;22195-519;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 840 WHITE_22195-520;320;1.8;4000;2300;Acrylic - Fagerhult - Delta Microprism;630;2300;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047637162;22195-520;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 840 WHITE_22195-528;320;1.8;4000;2300;Acrylic - Fagerhult - Delta Microprism;630;2300;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047637124;22195-528;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 840 WHITE_22195-529;320;1.8;4000;2300;Acrylic - Fagerhult - Delta Microprism;630;2300;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047637148;22195-529;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;0
DWIDE DELTA REC VTB 300X600 930 WHITE_22196;320;1.8;3000;1691;Acrylic - Fagerhult - Delta Microprism;630;1691;3000;3000;20;57;104;White;Aluminium - Fagerhult - White;7320047637179;22196;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 930 WHITE_22196-3;320;1.8;3000;1691;Acrylic - Fagerhult - Delta Microprism;630;1691;3000;3000;20;57;104;White;Aluminium - Fagerhult - White;7320047637186;22196-3;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 930 WHITE_22196-111;320;1.8;3000;1691;Acrylic - Fagerhult - Delta Microprism;630;1691;3000;3000;20;57;104;White;Aluminium - Fagerhult - White;7320047637209;22196-111;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 930 WHITE_22196-340;320;1.8;3000;1691;Acrylic - Fagerhult - Delta Microprism;630;1691;3000;3000;20;57;104;White;Aluminium - Fagerhult - White;7320047637223;22196-340;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 930 WHITE_22196-402;320;1.8;3000;1827;Acrylic - Fagerhult - Delta Microprism;630;1827;3000;3000;20;57;108;White;Aluminium - Fagerhult - White;7320047637193;22196-402;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 930 WHITE_22196-519;320;1.8;3000;1691;Acrylic - Fagerhult - Delta Microprism;630;1691;3000;3000;20;57;104;White;Aluminium - Fagerhult - White;7320047637247;22196-519;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 930 WHITE_22196-520;320;1.8;3000;1827;Acrylic - Fagerhult - Delta Microprism;630;1827;3000;3000;20;57;108;White;Aluminium - Fagerhult - White;7320047637254;22196-520;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 930 WHITE_22196-528;320;1.8;3000;1827;Acrylic - Fagerhult - Delta Microprism;630;1827;3000;3000;20;57;108;White;Aluminium - Fagerhult - White;7320047637216;22196-528;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 930 WHITE_22196-529;320;1.8;3000;1827;Acrylic - Fagerhult - Delta Microprism;630;1827;3000;3000;20;57;108;White;Aluminium - Fagerhult - White;7320047637230;22196-529;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 940 WHITE_22197;320;1.8;4000;1801;Acrylic - Fagerhult - Delta Microprism;630;1801;4000;4000;20;57;111;White;Aluminium - Fagerhult - White;7320047637285;22197;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 940 WHITE_22197-3;320;1.8;4000;1801;Acrylic - Fagerhult - Delta Microprism;630;1801;4000;4000;20;57;111;White;Aluminium - Fagerhult - White;7320047637315;22197-3;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 940 WHITE_22197-111;320;1.8;4000;1801;Acrylic - Fagerhult - Delta Microprism;630;1801;4000;4000;20;57;111;White;Aluminium - Fagerhult - White;7320047637346;22197-111;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 940 WHITE_22197-340;320;1.8;4000;1801;Acrylic - Fagerhult - Delta Microprism;630;1801;4000;4000;20;57;111;White;Aluminium - Fagerhult - White;7320047637360;22197-340;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 940 WHITE_22197-402;320;1.8;4000;1946;Acrylic - Fagerhult - Delta Microprism;630;1946;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047637339;22197-402;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 940 WHITE_22197-519;320;1.8;4000;1801;Acrylic - Fagerhult - Delta Microprism;630;1801;4000;4000;20;57;111;White;Aluminium - Fagerhult - White;7320047637384;22197-519;16;16;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 940 WHITE_22197-520;320;1.8;4000;1946;Acrylic - Fagerhult - Delta Microprism;630;1946;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047637391;22197-520;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 940 WHITE_22197-528;320;1.8;4000;1946;Acrylic - Fagerhult - Delta Microprism;630;1946;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047637353;22197-528;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 300X600 940 WHITE_22197-529;320;1.8;4000;1946;Acrylic - Fagerhult - Delta Microprism;630;1946;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047637377;22197-529;19;19;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;3;0
DWIDE DELTA REC VTB 600X600 HL 830 WHITE_22200;595;3.6;3000;4411;Acrylic - Fagerhult - Delta Microprism;595;4411;3000;3000;20;57;132;White;Aluminium - Fagerhult - White;7320047454608;22200;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 830 WHITE_22200-3;595;3.6;3000;4411;Acrylic - Fagerhult - Delta Microprism;595;4411;3000;3000;20;57;132;White;Aluminium - Fagerhult - White;7320047454622;22200-3;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 830 WHITE_22200-111;595;3.6;3000;4411;Acrylic - Fagerhult - Delta Microprism;595;4411;3000;3000;20;57;132;White;Aluminium - Fagerhult - White;7320047454646;22200-111;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 830 WHITE_22200-340;595;3.6;3000;4411;Acrylic - Fagerhult - Delta Microprism;595;4411;3000;3000;20;57;132;White;Aluminium - Fagerhult - White;7320047454660;22200-340;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 830 WHITE_22200-402;595;3.6;3000;4367;Acrylic - Fagerhult - Delta Microprism;595;4367;3000;3000;20;57;132;White;Aluminium - Fagerhult - White;7320047454707;22200-402;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 830 WHITE_22200-519;595;3.6;3000;4411;Acrylic - Fagerhult - Delta Microprism;595;4411;3000;3000;20;57;132;White;Aluminium - Fagerhult - White;7320047454684;22200-519;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 830 WHITE_22200-520;595;3.6;3000;4367;Acrylic - Fagerhult - Delta Microprism;595;4367;3000;3000;20;57;132;White;Aluminium - Fagerhult - White;7320047454769;22200-520;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 830 WHITE_22200-528;595;3.6;3000;4367;Acrylic - Fagerhult - Delta Microprism;595;4367;3000;3000;20;57;132;White;Aluminium - Fagerhult - White;7320047454721;22200-528;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 830 WHITE_22200-529;595;3.6;3000;4367;Acrylic - Fagerhult - Delta Microprism;595;4367;3000;3000;20;57;132;White;Aluminium - Fagerhult - White;7320047454745;22200-529;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 840 WHITE_22201;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;137;White;Aluminium - Fagerhult - White;7320047454783;22201;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 840 WHITE_22201-3;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;137;White;Aluminium - Fagerhult - White;7320047454806;22201-3;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 840 WHITE_22201-111;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;137;White;Aluminium - Fagerhult - White;7320047454820;22201-111;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 840 WHITE_22201-340;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;137;White;Aluminium - Fagerhult - White;7320047454844;22201-340;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 840 WHITE_22201-402;595;3.6;4000;4393;Acrylic - Fagerhult - Delta Microprism;595;4393;4000;4000;20;57;139;White;Aluminium - Fagerhult - White;7320047454882;22201-402;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 840 WHITE_22201-519;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;137;White;Aluminium - Fagerhult - White;7320047454868;22201-519;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 840 WHITE_22201-520;595;3.6;4000;4393;Acrylic - Fagerhult - Delta Microprism;595;4393;4000;4000;20;57;139;White;Aluminium - Fagerhult - White;7320047454943;22201-520;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 840 WHITE_22201-528;595;3.6;4000;4393;Acrylic - Fagerhult - Delta Microprism;595;4393;4000;4000;20;57;139;White;Aluminium - Fagerhult - White;7320047454905;22201-528;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 840 WHITE_22201-529;595;3.6;4000;4393;Acrylic - Fagerhult - Delta Microprism;595;4393;4000;4000;20;57;139;White;Aluminium - Fagerhult - White;7320047454929;22201-529;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 930 WHITE_22202;595;3.6;3000;3692;Acrylic - Fagerhult - Delta Microprism;595;3692;3000;3000;20;57;110;White;Aluminium - Fagerhult - White;7320047454967;22202;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 930 WHITE_22202-3;595;3.6;3000;3692;Acrylic - Fagerhult - Delta Microprism;595;3692;3000;3000;20;57;110;White;Aluminium - Fagerhult - White;7320047454981;22202-3;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 930 WHITE_22202-111;595;3.6;3000;3692;Acrylic - Fagerhult - Delta Microprism;595;3692;3000;3000;20;57;110;White;Aluminium - Fagerhult - White;7320047455001;22202-111;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 930 WHITE_22202-340;595;3.6;3000;3692;Acrylic - Fagerhult - Delta Microprism;595;3692;3000;3000;20;57;110;White;Aluminium - Fagerhult - White;7320047455025;22202-340;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 930 WHITE_22202-402;595;3.6;3000;3655;Acrylic - Fagerhult - Delta Microprism;595;3655;3000;3000;20;57;111;White;Aluminium - Fagerhult - White;7320047455063;22202-402;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 930 WHITE_22202-519;595;3.6;3000;3692;Acrylic - Fagerhult - Delta Microprism;595;3692;3000;3000;20;57;110;White;Aluminium - Fagerhult - White;7320047455049;22202-519;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 930 WHITE_22202-520;595;3.6;3000;3655;Acrylic - Fagerhult - Delta Microprism;595;3655;3000;3000;20;57;111;White;Aluminium - Fagerhult - White;7320047455124;22202-520;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 930 WHITE_22202-528;595;3.6;3000;3655;Acrylic - Fagerhult - Delta Microprism;595;3655;3000;3000;20;57;111;White;Aluminium - Fagerhult - White;7320047455087;22202-528;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 930 WHITE_22202-529;595;3.6;3000;3655;Acrylic - Fagerhult - Delta Microprism;595;3655;3000;3000;20;57;111;White;Aluminium - Fagerhult - White;7320047455100;22202-529;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 940 WHITE_22203;595;3.6;4000;3714;Acrylic - Fagerhult - Delta Microprism;595;3714;4000;4000;20;57;116;White;Aluminium - Fagerhult - White;7320047455148;22203;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 940 WHITE_22203-3;595;3.6;4000;3714;Acrylic - Fagerhult - Delta Microprism;595;3714;4000;4000;20;57;116;White;Aluminium - Fagerhult - White;7320047455162;22203-3;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 940 WHITE_22203-111;595;3.6;4000;3714;Acrylic - Fagerhult - Delta Microprism;595;3714;4000;4000;20;57;116;White;Aluminium - Fagerhult - White;7320047455186;22203-111;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 940 WHITE_22203-340;595;3.6;4000;3714;Acrylic - Fagerhult - Delta Microprism;595;3714;4000;4000;20;57;116;White;Aluminium - Fagerhult - White;7320047455209;22203-340;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 940 WHITE_22203-402;595;3.6;4000;3716;Acrylic - Fagerhult - Delta Microprism;595;3716;4000;4000;20;57;118;White;Aluminium - Fagerhult - White;7320047455247;22203-402;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 940 WHITE_22203-519;595;3.6;4000;3714;Acrylic - Fagerhult - Delta Microprism;595;3714;4000;4000;20;57;116;White;Aluminium - Fagerhult - White;7320047455223;22203-519;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 940 WHITE_22203-520;595;3.6;4000;3716;Acrylic - Fagerhult - Delta Microprism;595;3716;4000;4000;20;57;118;White;Aluminium - Fagerhult - White;7320047455308;22203-520;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 940 WHITE_22203-528;595;3.6;4000;3716;Acrylic - Fagerhult - Delta Microprism;595;3716;4000;4000;20;57;118;White;Aluminium - Fagerhult - White;7320047455261;22203-528;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 HL 940 WHITE_22203-529;595;3.6;4000;3716;Acrylic - Fagerhult - Delta Microprism;595;3716;4000;4000;20;57;118;White;Aluminium - Fagerhult - White;7320047455285;22203-529;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 300X1200 HL 830 WHITE_22205;296;3.5;3000;4373;Acrylic - Fagerhult - Delta Microprism;1196;4373;3000;3000;20;57;131;White;Aluminium - Fagerhult - White;7320047455322;22205;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 830 WHITE_22205-3;296;3.5;3000;4373;Acrylic - Fagerhult - Delta Microprism;1196;4373;3000;3000;20;57;131;White;Aluminium - Fagerhult - White;7320047455346;22205-3;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 830 WHITE_22205-111;296;3.5;3000;4373;Acrylic - Fagerhult - Delta Microprism;1196;4373;3000;3000;20;57;131;White;Aluminium - Fagerhult - White;7320047455360;22205-111;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 830 WHITE_22205-340;296;3.5;3000;4373;Acrylic - Fagerhult - Delta Microprism;1196;4373;3000;3000;20;57;131;White;Aluminium - Fagerhult - White;7320047455384;22205-340;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 830 WHITE_22205-402;296;3.5;3000;4329;Acrylic - Fagerhult - Delta Microprism;1196;4329;3000;3000;20;57;131;White;Aluminium - Fagerhult - White;7320047455421;22205-402;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 830 WHITE_22205-519;296;3.5;3000;4373;Acrylic - Fagerhult - Delta Microprism;1196;4373;3000;3000;20;57;131;White;Aluminium - Fagerhult - White;7320047455407;22205-519;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 830 WHITE_22205-520;296;3.5;3000;4329;Acrylic - Fagerhult - Delta Microprism;1196;4329;3000;3000;20;57;131;White;Aluminium - Fagerhult - White;7320047455483;22205-520;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 830 WHITE_22205-528;296;3.5;3000;4329;Acrylic - Fagerhult - Delta Microprism;1196;4329;3000;3000;20;57;131;White;Aluminium - Fagerhult - White;7320047455445;22205-528;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 830 WHITE_22205-529;296;3.5;3000;4329;Acrylic - Fagerhult - Delta Microprism;1196;4329;3000;3000;20;57;131;White;Aluminium - Fagerhult - White;7320047455469;22205-529;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 840 WHITE_22206;296;3.5;4000;4352;Acrylic - Fagerhult - Delta Microprism;1196;4352;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047455506;22206;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 840 WHITE_22206-3;296;3.5;4000;4352;Acrylic - Fagerhult - Delta Microprism;1196;4352;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047455520;22206-3;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 840 WHITE_22206-111;296;3.5;4000;4352;Acrylic - Fagerhult - Delta Microprism;1196;4352;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047455544;22206-111;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 840 WHITE_22206-340;296;3.5;4000;4352;Acrylic - Fagerhult - Delta Microprism;1196;4352;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047455568;22206-340;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 840 WHITE_22206-402;296;3.5;4000;4355;Acrylic - Fagerhult - Delta Microprism;1196;4355;4000;4000;20;57;138;White;Aluminium - Fagerhult - White;7320047455605;22206-402;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 840 WHITE_22206-519;296;3.5;4000;4352;Acrylic - Fagerhult - Delta Microprism;1196;4352;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047455582;22206-519;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 840 WHITE_22206-520;296;3.5;4000;4355;Acrylic - Fagerhult - Delta Microprism;1196;4355;4000;4000;20;57;138;White;Aluminium - Fagerhult - White;7320047455667;22206-520;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 840 WHITE_22206-528;296;3.5;4000;4355;Acrylic - Fagerhult - Delta Microprism;1196;4355;4000;4000;20;57;138;White;Aluminium - Fagerhult - White;7320047455629;22206-528;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 840 WHITE_22206-529;296;3.5;4000;4355;Acrylic - Fagerhult - Delta Microprism;1196;4355;4000;4000;20;57;138;White;Aluminium - Fagerhult - White;7320047455643;22206-529;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 930 WHITE_22207;296;3.5;3000;3660;Acrylic - Fagerhult - Delta Microprism;1196;3660;3000;3000;20;57;109;White;Aluminium - Fagerhult - White;7320047478604;22207;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 930 WHITE_22207-3;296;3.5;3000;3660;Acrylic - Fagerhult - Delta Microprism;1196;3660;3000;3000;20;57;109;White;Aluminium - Fagerhult - White;7320047478628;22207-3;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 930 WHITE_22207-111;296;3.5;3000;3660;Acrylic - Fagerhult - Delta Microprism;1196;3660;3000;3000;20;57;109;White;Aluminium - Fagerhult - White;7320047478642;22207-111;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 930 WHITE_22207-340;296;3.5;3000;3660;Acrylic - Fagerhult - Delta Microprism;1196;3660;3000;3000;20;57;109;White;Aluminium - Fagerhult - White;7320047478666;22207-340;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 930 WHITE_22207-402;296;3.5;3000;3624;Acrylic - Fagerhult - Delta Microprism;1196;3624;3000;3000;20;57;110;White;Aluminium - Fagerhult - White;7320047478703;22207-402;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 930 WHITE_22207-519;296;3.5;3000;3660;Acrylic - Fagerhult - Delta Microprism;1196;3660;3000;3000;20;57;109;White;Aluminium - Fagerhult - White;7320047478680;22207-519;34;34;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 930 WHITE_22207-520;296;3.5;3000;3624;Acrylic - Fagerhult - Delta Microprism;1196;3624;3000;3000;20;57;110;White;Aluminium - Fagerhult - White;7320047478765;22207-520;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 930 WHITE_22207-528;296;3.5;3000;3624;Acrylic - Fagerhult - Delta Microprism;1196;3624;3000;3000;20;57;110;White;Aluminium - Fagerhult - White;7320047478727;22207-528;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 930 WHITE_22207-529;296;3.5;3000;3624;Acrylic - Fagerhult - Delta Microprism;1196;3624;3000;3000;20;57;110;White;Aluminium - Fagerhult - White;7320047478741;22207-529;37;37;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 940 WHITE_22208;296;3.5;4000;3682;Acrylic - Fagerhult - Delta Microprism;1196;3682;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047478789;22208;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 940 WHITE_22208-3;296;3.5;4000;3682;Acrylic - Fagerhult - Delta Microprism;1196;3682;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047478802;22208-3;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 940 WHITE_22208-111;296;3.5;4000;3682;Acrylic - Fagerhult - Delta Microprism;1196;3682;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047478826;22208-111;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 940 WHITE_22208-340;296;3.5;4000;3682;Acrylic - Fagerhult - Delta Microprism;1196;3682;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047478840;22208-340;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 940 WHITE_22208-402;296;3.5;4000;3684;Acrylic - Fagerhult - Delta Microprism;1196;3684;4000;4000;20;57;117;White;Aluminium - Fagerhult - White;7320047478888;22208-402;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 940 WHITE_22208-519;296;3.5;4000;3682;Acrylic - Fagerhult - Delta Microprism;1196;3682;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047478864;22208-519;32;32;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 940 WHITE_22208-520;296;3.5;4000;3684;Acrylic - Fagerhult - Delta Microprism;1196;3684;4000;4000;20;57;117;White;Aluminium - Fagerhult - White;7320047478949;22208-520;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 940 WHITE_22208-528;296;3.5;4000;3684;Acrylic - Fagerhult - Delta Microprism;1196;3684;4000;4000;20;57;117;White;Aluminium - Fagerhult - White;7320047478901;22208-528;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 HL 940 WHITE_22208-529;296;3.5;4000;3684;Acrylic - Fagerhult - Delta Microprism;1196;3684;4000;4000;20;57;117;White;Aluminium - Fagerhult - White;7320047478925;22208-529;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 600X600 LL 830 WHITE_22500;595;3.5;3000;3010;Acrylic - Fagerhult - Delta Microprism;595;3010;3000;3000;20;57;134;White;Aluminium - Fagerhult - White;7320047481246;22500;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 830 WHITE_22500-3;595;3.5;3000;3010;Acrylic - Fagerhult - Delta Microprism;595;3010;3000;3000;20;57;134;White;Aluminium - Fagerhult - White;7320047481260;22500-3;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 830 WHITE_22500-111;595;3.5;3000;3010;Acrylic - Fagerhult - Delta Microprism;595;3010;3000;3000;20;57;134;White;Aluminium - Fagerhult - White;7320047481284;22500-111;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 830 WHITE_22500-340;595;3.5;3000;3010;Acrylic - Fagerhult - Delta Microprism;595;3010;3000;3000;20;57;134;White;Aluminium - Fagerhult - White;7320047481307;22500-340;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 830 WHITE_22500-402;595;3.5;3000;3047;Acrylic - Fagerhult - Delta Microprism;595;3047;3000;3000;20;57;137;White;Aluminium - Fagerhult - White;7320047481345;22500-402;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 830 WHITE_22500-519;595;3.5;3000;3010;Acrylic - Fagerhult - Delta Microprism;595;3010;3000;3000;20;57;134;White;Aluminium - Fagerhult - White;7320047481321;22500-519;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 830 WHITE_22500-520;595;3.5;3000;3047;Acrylic - Fagerhult - Delta Microprism;595;3047;3000;3000;20;57;137;White;Aluminium - Fagerhult - White;7320047481406;22500-520;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 830 WHITE_22500-528;595;3.5;3000;3047;Acrylic - Fagerhult - Delta Microprism;595;3047;3000;3000;20;57;137;White;Aluminium - Fagerhult - White;7320047481369;22500-528;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 830 WHITE_22500-529;595;3.5;3000;3047;Acrylic - Fagerhult - Delta Microprism;595;3047;3000;3000;20;57;137;White;Aluminium - Fagerhult - White;7320047481383;22500-529;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 840 WHITE_22501;595;3.5;4000;2907;Acrylic - Fagerhult - Delta Microprism;595;2907;4000;4000;20;57;140;White;Aluminium - Fagerhult - White;7320047481420;22501;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 840 WHITE_22501-3;595;3.5;4000;2907;Acrylic - Fagerhult - Delta Microprism;595;2907;4000;4000;20;57;140;White;Aluminium - Fagerhult - White;7320047481444;22501-3;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 840 WHITE_22501-111;595;3.5;4000;2907;Acrylic - Fagerhult - Delta Microprism;595;2907;4000;4000;20;57;140;White;Aluminium - Fagerhult - White;7320047481468;22501-111;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 840 WHITE_22501-340;595;3.5;4000;2907;Acrylic - Fagerhult - Delta Microprism;595;2907;4000;4000;20;57;140;White;Aluminium - Fagerhult - White;7320047481482;22501-340;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 840 WHITE_22501-402;595;3.5;4000;2997;Acrylic - Fagerhult - Delta Microprism;595;2997;4000;4000;20;57;143;White;Aluminium - Fagerhult - White;7320047481529;22501-402;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 840 WHITE_22501-519;595;3.5;4000;2907;Acrylic - Fagerhult - Delta Microprism;595;2907;4000;4000;20;57;140;White;Aluminium - Fagerhult - White;7320047481505;22501-519;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 840 WHITE_22501-520;595;3.5;4000;2997;Acrylic - Fagerhult - Delta Microprism;595;2997;4000;4000;20;57;143;White;Aluminium - Fagerhult - White;7320047481581;22501-520;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 840 WHITE_22501-528;595;3.5;4000;2997;Acrylic - Fagerhult - Delta Microprism;595;2997;4000;4000;20;57;143;White;Aluminium - Fagerhult - White;7320047481543;22501-528;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 840 WHITE_22501-529;595;3.5;4000;2997;Acrylic - Fagerhult - Delta Microprism;595;2997;4000;4000;20;57;143;White;Aluminium - Fagerhult - White;7320047481567;22501-529;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 LL 930 WHITE_22502;595;3.5;3000;2519;Acrylic - Fagerhult - Delta Microprism;595;2519;3000;3000;20;57;112;White;Aluminium - Fagerhult - White;7320047481604;22502;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 930 WHITE_22502-3;595;3.5;3000;2519;Acrylic - Fagerhult - Delta Microprism;595;2519;3000;3000;20;57;112;White;Aluminium - Fagerhult - White;7320047481628;22502-3;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 930 WHITE_22502-111;595;3.5;3000;2519;Acrylic - Fagerhult - Delta Microprism;595;2519;3000;3000;20;57;112;White;Aluminium - Fagerhult - White;7320047481642;22502-111;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 930 WHITE_22502-340;595;3.5;3000;2519;Acrylic - Fagerhult - Delta Microprism;595;2519;3000;3000;20;57;112;White;Aluminium - Fagerhult - White;7320047481666;22502-340;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 930 WHITE_22502-402;595;3.5;3000;2550;Acrylic - Fagerhult - Delta Microprism;595;2550;3000;3000;20;57;114;White;Aluminium - Fagerhult - White;7320047481703;22502-402;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 930 WHITE_22502-519;595;3.5;3000;2519;Acrylic - Fagerhult - Delta Microprism;595;2519;3000;3000;20;57;112;White;Aluminium - Fagerhult - White;7320047481680;22502-519;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 930 WHITE_22502-520;595;3.5;3000;2550;Acrylic - Fagerhult - Delta Microprism;595;2550;3000;3000;20;57;114;White;Aluminium - Fagerhult - White;7320047481765;22502-520;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 930 WHITE_22502-528;595;3.5;3000;2550;Acrylic - Fagerhult - Delta Microprism;595;2550;3000;3000;20;57;114;White;Aluminium - Fagerhult - White;7320047481727;22502-528;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 930 WHITE_22502-529;595;3.5;3000;2550;Acrylic - Fagerhult - Delta Microprism;595;2550;3000;3000;20;57;114;White;Aluminium - Fagerhult - White;7320047481741;22502-529;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 940 WHITE_22503;595;3.5;4000;2459;Acrylic - Fagerhult - Delta Microprism;595;2459;4000;4000;20;57;119;White;Aluminium - Fagerhult - White;7320047481789;22503;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 940 WHITE_22503-3;595;3.5;4000;2459;Acrylic - Fagerhult - Delta Microprism;595;2459;4000;4000;20;57;119;White;Aluminium - Fagerhult - White;7320047481802;22503-3;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 940 WHITE_22503-111;595;3.5;4000;2459;Acrylic - Fagerhult - Delta Microprism;595;2459;4000;4000;20;57;119;White;Aluminium - Fagerhult - White;7320047481826;22503-111;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 940 WHITE_22503-340;595;3.5;4000;2459;Acrylic - Fagerhult - Delta Microprism;595;2459;4000;4000;20;57;119;White;Aluminium - Fagerhult - White;7320047481840;22503-340;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 940 WHITE_22503-402;595;3.5;4000;2535;Acrylic - Fagerhult - Delta Microprism;595;2535;4000;4000;20;57;121;White;Aluminium - Fagerhult - White;7320047481888;22503-402;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 940 WHITE_22503-519;595;3.5;4000;2459;Acrylic - Fagerhult - Delta Microprism;595;2459;4000;4000;20;57;119;White;Aluminium - Fagerhult - White;7320047481864;22503-519;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 940 WHITE_22503-520;595;3.5;4000;2535;Acrylic - Fagerhult - Delta Microprism;595;2535;4000;4000;20;57;121;White;Aluminium - Fagerhult - White;7320047481949;22503-520;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 940 WHITE_22503-528;595;3.5;4000;2535;Acrylic - Fagerhult - Delta Microprism;595;2535;4000;4000;20;57;121;White;Aluminium - Fagerhult - White;7320047481901;22503-528;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 600X600 LL 940 WHITE_22503-529;595;3.5;4000;2535;Acrylic - Fagerhult - Delta Microprism;595;2535;4000;4000;20;57;121;White;Aluminium - Fagerhult - White;7320047481925;22503-529;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;2;0
DWIDE DELTA REC VTB 300X1200 LL 830 WHITE_22505;296;3.5;3000;2983;Acrylic - Fagerhult - Delta Microprism;1196;2983;3000;3000;20;57;133;White;Aluminium - Fagerhult - White;7320047481963;22505;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 830 WHITE_22505-3;296;3.5;3000;2983;Acrylic - Fagerhult - Delta Microprism;1196;2983;3000;3000;20;57;133;White;Aluminium - Fagerhult - White;7320047481987;22505-3;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 830 WHITE_22505-111;296;3.5;3000;2983;Acrylic - Fagerhult - Delta Microprism;1196;2983;3000;3000;20;57;133;White;Aluminium - Fagerhult - White;7320047482007;22505-111;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 830 WHITE_22505-340;296;3.5;3000;2983;Acrylic - Fagerhult - Delta Microprism;1196;2983;3000;3000;20;57;133;White;Aluminium - Fagerhult - White;7320047482021;22505-340;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 830 WHITE_22505-402;296;3.5;3000;3021;Acrylic - Fagerhult - Delta Microprism;1196;3021;3000;3000;20;57;135;White;Aluminium - Fagerhult - White;7320047482069;22505-402;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 830 WHITE_22505-519;296;3.5;3000;2983;Acrylic - Fagerhult - Delta Microprism;1196;2983;3000;3000;20;57;133;White;Aluminium - Fagerhult - White;7320047482045;22505-519;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 830 WHITE_22505-520;296;3.5;3000;3021;Acrylic - Fagerhult - Delta Microprism;1196;3021;3000;3000;20;57;135;White;Aluminium - Fagerhult - White;7320047482120;22505-520;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 830 WHITE_22505-528;296;3.5;3000;3021;Acrylic - Fagerhult - Delta Microprism;1196;3021;3000;3000;20;57;135;White;Aluminium - Fagerhult - White;7320047482083;22505-528;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 830 WHITE_22505-529;296;3.5;3000;3021;Acrylic - Fagerhult - Delta Microprism;1196;3021;3000;3000;20;57;135;White;Aluminium - Fagerhult - White;7320047482106;22505-529;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 840 WHITE_22506;296;3.5;4000;2882;Acrylic - Fagerhult - Delta Microprism;1196;2882;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047482144;22506;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 840 WHITE_22506-3;296;3.5;4000;2882;Acrylic - Fagerhult - Delta Microprism;1196;2882;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047482168;22506-3;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 840 WHITE_22506-111;296;3.5;4000;2882;Acrylic - Fagerhult - Delta Microprism;1196;2882;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047482182;22506-111;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 840 WHITE_22506-340;296;3.5;4000;2882;Acrylic - Fagerhult - Delta Microprism;1196;2882;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047482205;22506-340;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 840 WHITE_22506-402;296;3.5;4000;2971;Acrylic - Fagerhult - Delta Microprism;1196;2971;4000;4000;20;57;138;White;Aluminium - Fagerhult - White;7320047482243;22506-402;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 840 WHITE_22506-519;296;3.5;4000;2882;Acrylic - Fagerhult - Delta Microprism;1196;2882;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7320047482229;22506-519;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 840 WHITE_22506-520;296;3.5;4000;2971;Acrylic - Fagerhult - Delta Microprism;1196;2971;4000;4000;20;57;138;White;Aluminium - Fagerhult - White;7320047482304;22506-520;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 840 WHITE_22506-528;296;3.5;4000;2971;Acrylic - Fagerhult - Delta Microprism;1196;2971;4000;4000;20;57;138;White;Aluminium - Fagerhult - White;7320047482267;22506-528;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 840 WHITE_22506-529;296;3.5;4000;2971;Acrylic - Fagerhult - Delta Microprism;1196;2971;4000;4000;20;57;138;White;Aluminium - Fagerhult - White;7320047482281;22506-529;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 930 WHITE_22507;296;3.5;3000;2497;Acrylic - Fagerhult - Delta Microprism;1196;2497;3000;3000;20;57;111;White;Aluminium - Fagerhult - White;7320047482328;22507;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 930 WHITE_22507-3;296;3.5;3000;2497;Acrylic - Fagerhult - Delta Microprism;1196;2497;3000;3000;20;57;111;White;Aluminium - Fagerhult - White;7320047482342;22507-3;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 930 WHITE_22507-111;296;3.5;3000;2497;Acrylic - Fagerhult - Delta Microprism;1196;2497;3000;3000;20;57;111;White;Aluminium - Fagerhult - White;7320047482366;22507-111;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 930 WHITE_22507-340;296;3.5;3000;2497;Acrylic - Fagerhult - Delta Microprism;1196;2497;3000;3000;20;57;111;White;Aluminium - Fagerhult - White;7320047482380;22507-340;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 930 WHITE_22507-402;296;3.5;3000;2528;Acrylic - Fagerhult - Delta Microprism;1196;2528;3000;3000;20;57;113;White;Aluminium - Fagerhult - White;7320047482427;22507-402;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 930 WHITE_22507-519;296;3.5;3000;2497;Acrylic - Fagerhult - Delta Microprism;1196;2497;3000;3000;20;57;111;White;Aluminium - Fagerhult - White;7320047482403;22507-519;23;23;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 930 WHITE_22507-520;296;3.5;3000;2528;Acrylic - Fagerhult - Delta Microprism;1196;2528;3000;3000;20;57;113;White;Aluminium - Fagerhult - White;7320047482489;22507-520;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 930 WHITE_22507-528;296;3.5;3000;2528;Acrylic - Fagerhult - Delta Microprism;1196;2528;3000;3000;20;57;113;White;Aluminium - Fagerhult - White;7320047482441;22507-528;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 930 WHITE_22507-529;296;3.5;3000;2528;Acrylic - Fagerhult - Delta Microprism;1196;2528;3000;3000;20;57;113;White;Aluminium - Fagerhult - White;7320047482465;22507-529;25;25;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 940 WHITE_22508;296;3.5;4000;2438;Acrylic - Fagerhult - Delta Microprism;1196;2438;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047482502;22508;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 940 WHITE_22508-3;296;3.5;4000;2438;Acrylic - Fagerhult - Delta Microprism;1196;2438;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047482526;22508-3;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 940 WHITE_22508-111;296;3.5;4000;2438;Acrylic - Fagerhult - Delta Microprism;1196;2438;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047482540;22508-111;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 940 WHITE_22508-340;296;3.5;4000;2438;Acrylic - Fagerhult - Delta Microprism;1196;2438;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047482564;22508-340;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 940 WHITE_22508-402;296;3.5;4000;2513;Acrylic - Fagerhult - Delta Microprism;1196;2513;4000;4000;20;57;117;White;Aluminium - Fagerhult - White;7320047482601;22508-402;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 940 WHITE_22508-519;296;3.5;4000;2438;Acrylic - Fagerhult - Delta Microprism;1196;2438;4000;4000;20;57;115;White;Aluminium - Fagerhult - White;7320047482588;22508-519;21;21;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 940 WHITE_22508-520;296;3.5;4000;2513;Acrylic - Fagerhult - Delta Microprism;1196;2513;4000;4000;20;57;117;White;Aluminium - Fagerhult - White;7320047482663;22508-520;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 940 WHITE_22508-528;296;3.5;4000;2513;Acrylic - Fagerhult - Delta Microprism;1196;2513;4000;4000;20;57;117;White;Aluminium - Fagerhult - White;7320047482625;22508-528;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 300X1200 LL 940 WHITE_22508-529;296;3.5;4000;2513;Acrylic - Fagerhult - Delta Microprism;1196;2513;4000;4000;20;57;117;White;Aluminium - Fagerhult - White;7320047482649;22508-529;23.5;23.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;D;3;1;0
DWIDE DELTA REC VTB 600X600 HL 830 WHITE_22200-546;595;4.2;3000;4367;Acrylic - Fagerhult - Delta Microprism;595;4367;3000;3000;20;56;128;White;Aluminium - Fagerhult - White;7320048522016;22200-546;38;38;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 HL 840 WHITE_22201-546;595;4.2;4000;4393;Acrylic - Fagerhult - Delta Microprism;595;4393;4000;4000;20;56;134;White;Aluminium - Fagerhult - White;7320048522030;22201-546;36.5;36.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;0
DWIDE DELTA REC VTB 600X600 TW OR WHITE_22214;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;102;White;Aluminium - Fagerhult - White;7316910002212;22214;43.5;43.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;E;3;2;1
DWIDE DELTA REC VTB 600X600 TW OR WHITE_22214-3;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;102;White;Aluminium - Fagerhult - White;7316910002236;22214-3;44.5;44.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;E;3;2;1
DWIDE DELTA REC VTB 600X600 TW OR WHITE_22214-340;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;102;White;Aluminium - Fagerhult - White;7316911441553;22214-340;44.5;44.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;E;3;2;1
DWIDE DELTA REC VTB 600X600 TW OR WHITE_22214-111;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;102;White;Aluminium - Fagerhult - White;7316911441546;22214-111;44.5;44.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;E;3;2;1
DWIDE DELTA REC VTB 600X600 TW OR WHITE_22214-519;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;102;White;Aluminium - Fagerhult - White;7316911441560;22214-519;44.5;44.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;E;3;2;1
DWIDE DELTA REC VTB 600X600 830 OR WHITE_22300;595;3.6;3000;4367;Acrylic - Fagerhult - Delta Microprism;595;4367;3000;3000;20;57;132;White;Aluminium - Fagerhult - White;7316911438065;22300;37.5;37.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;1
DWIDE DELTA REC VTB 600X600 830 OR WHITE_22300-111;595;3.6;3000;4367;Acrylic - Fagerhult - Delta Microprism;595;4367;3000;3000;20;57;130;White;Aluminium - Fagerhult - White;7316911441577;22300-111;37.5;37.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;1
DWIDE DELTA REC VTB 600X600 830 OR WHITE_22300-3;595;3.6;3000;4367;Acrylic - Fagerhult - Delta Microprism;595;4367;3000;3000;20;57;132;White;Aluminium - Fagerhult - White;7316911441584;22300-3;37.5;37.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;1
DWIDE DELTA REC VTB 600X600 830 OR WHITE_22300-340;595;3.6;3000;4367;Acrylic - Fagerhult - Delta Microprism;595;4367;3000;3000;20;57;130;White;Aluminium - Fagerhult - White;7316911441591;22300-340;37.5;37.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;1
DWIDE DELTA REC VTB 600X600 830 OR WHITE_22300-519;595;3.6;3000;4367;Acrylic - Fagerhult - Delta Microprism;595;4367;3000;3000;20;57;130;White;Aluminium - Fagerhult - White;7316911441607;22300-519;37.5;37.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;1
DWIDE DELTA REC VTB 600X600 840 OR WHITE_22301;595;3.6;4000;4393;Acrylic - Fagerhult - Delta Microprism;595;4393;4000;4000;20;57;138;White;Aluminium - Fagerhult - White;7316911438164;22301;36;36;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;1
DWIDE DELTA REC VTB 600X600 840 OR WHITE_22301-111;595;3.6;4000;4393;Acrylic - Fagerhult - Delta Microprism;595;4393;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7316911441614;22301-111;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;1
DWIDE DELTA REC VTB 600X600 840 OR WHITE_22301-3;595;3.6;4000;4393;Acrylic - Fagerhult - Delta Microprism;595;4393;4000;4000;20;57;138;White;Aluminium - Fagerhult - White;7316911441621;22301-3;36;36;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;1
DWIDE DELTA REC VTB 600X600 840 OR WHITE_22301-340;595;3.6;4000;4393;Acrylic - Fagerhult - Delta Microprism;595;4393;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7316911441638;22301-340;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;1
DWIDE DELTA REC VTB 600X600 840 OR WHITE_22301-519;595;3.6;4000;4393;Acrylic - Fagerhult - Delta Microprism;595;4393;4000;4000;20;57;136;White;Aluminium - Fagerhult - White;7316911441645;22301-519;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;2;1
DWIDE DELTA REC VTB 300X600 830 OR WHITE_22302;296;1.6;3000;2183;Acrylic - Fagerhult - Delta Microprism;595;2183;3000;3000;20;57;122;White;Aluminium - Fagerhult - White;7316911438263;22302;20;20;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;2
DWIDE DELTA REC VTB 300X600 830 OR WHITE_22302-111;296;1.6;3000;2183;Acrylic - Fagerhult - Delta Microprism;595;2183;3000;3000;20;57;121;White;Aluminium - Fagerhult - White;7316911441652;22302-111;20;20;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;2
DWIDE DELTA REC VTB 300X600 830 OR WHITE_22302-3;296;1.6;3000;2183;Acrylic - Fagerhult - Delta Microprism;595;2183;3000;3000;20;57;122;White;Aluminium - Fagerhult - White;7316911441669;22302-3;20;20;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;2
DWIDE DELTA REC VTB 300X600 830 OR WHITE_22302-340;296;1.6;3000;2183;Acrylic - Fagerhult - Delta Microprism;595;2183;3000;3000;20;57;121;White;Aluminium - Fagerhult - White;7316911441720;22302-340;20;20;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;2
DWIDE DELTA REC VTB 300X600 830 OR WHITE_22302-519;296;1.6;3000;2183;Acrylic - Fagerhult - Delta Microprism;595;2183;3000;3000;20;57;121;White;Aluminium - Fagerhult - White;7316911441737;22302-519;20;20;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;2
DWIDE DELTA REC VTB 300X600 840 OR WHITE_22303;296;1.6;4000;2300;Acrylic - Fagerhult - Delta Microprism;595;2300;4000;4000;20;57;129;White;Aluminium - Fagerhult - White;7316911438362;22303;20;20;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;2
DWIDE DELTA REC VTB 300X600 840 OR WHITE_22303-111;296;1.6;4000;2300;Acrylic - Fagerhult - Delta Microprism;595;2300;4000;4000;20;57;128;White;Aluminium - Fagerhult - White;7316911441744;22303-111;20;20;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;2
DWIDE DELTA REC VTB 300X600 840 OR WHITE_22303-3;296;1.6;4000;2300;Acrylic - Fagerhult - Delta Microprism;595;2300;4000;4000;20;57;129;White;Aluminium - Fagerhult - White;7316911441751;22303-3;20;20;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;2
DWIDE DELTA REC VTB 300X600 840 OR WHITE_22303-340;296;1.6;4000;2300;Acrylic - Fagerhult - Delta Microprism;595;2300;4000;4000;20;57;128;White;Aluminium - Fagerhult - White;7316911441768;22303-340;20;20;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;2
DWIDE DELTA REC VTB 300X600 840 OR WHITE_22303-519;296;1.6;4000;2300;Acrylic - Fagerhult - Delta Microprism;595;2300;4000;4000;20;57;128;White;Aluminium - Fagerhult - White;7316911441775;22303-519;20;20;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;3;2
DWIDE DELTA REC VTB 300X1200 830 OR WHITE_22304;296;3;3000;4329;Acrylic - Fagerhult - Delta Microprism;1196;4329;3000;3000;20;57;130;White;Aluminium - Fagerhult - White;7316911438461;22304;37.5;37.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;2
DWIDE DELTA REC VTB 300X1200 830 OR WHITE_22304-111;296;3;3000;4329;Acrylic - Fagerhult - Delta Microprism;1196;4329;3000;3000;20;57;129;White;Aluminium - Fagerhult - White;7316911441782;22304-111;37.5;37.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;2
DWIDE DELTA REC VTB 300X1200 830 OR WHITE_22304-3;296;3;3000;4329;Acrylic - Fagerhult - Delta Microprism;1196;4329;3000;3000;20;57;130;White;Aluminium - Fagerhult - White;7316911441799;22304-3;37.5;37.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;2
DWIDE DELTA REC VTB 300X1200 830 OR WHITE_22304-340;296;3;3000;4329;Acrylic - Fagerhult - Delta Microprism;1196;4329;3000;3000;20;57;129;White;Aluminium - Fagerhult - White;7316911441805;22304-340;37.5;37.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;2
DWIDE DELTA REC VTB 300X1200 830 OR WHITE_22304-519;296;3;3000;4329;Acrylic - Fagerhult - Delta Microprism;1196;4329;3000;3000;20;57;129;White;Aluminium - Fagerhult - White;7316911441812;22304-519;37.5;37.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;2
DWIDE DELTA REC VTB 300X1200 840 OR WHITE_22305;296;3;4000;4355;Acrylic - Fagerhult - Delta Microprism;1196;4355;4000;4000;20;57;137;White;Aluminium - Fagerhult - White;7316911438560;22305;36;36;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;2
DWIDE DELTA REC VTB 300X1200 840 OR WHITE_22305-111;296;3;4000;4355;Acrylic - Fagerhult - Delta Microprism;1196;4355;4000;4000;20;57;135;White;Aluminium - Fagerhult - White;7316911441829;22305-111;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;2
DWIDE DELTA REC VTB 300X1200 840 OR WHITE_22305-3;296;3;4000;4355;Acrylic - Fagerhult - Delta Microprism;1196;4355;4000;4000;20;57;137;White;Aluminium - Fagerhult - White;7316911441836;22305-3;36;36;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;2
DWIDE DELTA REC VTB 300X1200 840 OR WHITE_22305-340;296;3;4000;4355;Acrylic - Fagerhult - Delta Microprism;1196;4355;4000;4000;20;57;135;White;Aluminium - Fagerhult - White;7316911441843;22305-340;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;2
DWIDE DELTA REC VTB 300X1200 840 OR WHITE_22305-519;296;3;4000;4355;Acrylic - Fagerhult - Delta Microprism;1196;4355;4000;4000;20;57;135;White;Aluminium - Fagerhult - White;7316911441850;22305-519;35.5;35.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 80;C;3;1;2
DWIDE DELTA REC VTB 600X600 TW WHITE_22306;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;105;White;Aluminium - Fagerhult - White;7316911438669;22306;43.5;43.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;E;3;2;0
DWIDE DELTA REC VTB 600X600 TW WHITE_22306-528;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;105;White;Aluminium - Fagerhult - White;7316911438683;22306-528;43.5;43.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;E;3;2;0
DWIDE DELTA REC VTB 600X600 TW WHITE_22306-529;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;105;White;Aluminium - Fagerhult - White;7316911438706;22306-529;43.5;43.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;E;3;2;0
DWIDE DELTA REC VTB 600X600 TW WHITE_22306-520;595;3.6;4000;4390;Acrylic - Fagerhult - Delta Microprism;595;4390;4000;4000;20;57;105;White;Aluminium - Fagerhult - White;7316911438720;22306-520;43.5;43.5;Dwide recessed;Recessed mounting in suspended ceilings. Unventilated or ventilated ceilings.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm.</br><br><i>HB</i> – recessed frame allows 600x600 to be installed in suspended ceilings with concealed T-bars and symmetrical ceiling tiles (thickness 20-22 mm).;Recessed workplace luminaire in three sizes. The delta louvre provides efficiency and optimal light comfort, light divider in acrylic distributes light evenly in the reflector.;min. 90;E;3;2;0
