;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Type##OTHER##;Sensor##OTHER##
HERO 18KLM NARROW 4000K HTG_31504-525;307;7.3;4000;18118;589;18118;4000;4000;65;102;147;Black;Aluminium - Fagerhult - Black;7320047243011;31504-525;128.5;128.5;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;1
HERO 12KLM NARROW 4000K HTG_31499;307;7.3;4000;12048;498;12048;4000;4000;66;87;147;Black;Aluminium - Fagerhult - Black;7320046433420;31499;82;82;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;0
HERO 12KLM NARROW 4000K HTG_31499-461;307;7.3;4000;12048;498;12048;4000;4000;66;87;148;Black;Aluminium - Fagerhult - Black;7320046433444;31499-461;85;85;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;0
HERO 12KLM NARROW 4000K HTG_31499-525;307;7.3;4000;12048;589;12048;4000;4000;65;102;146;Black;Aluminium - Fagerhult - Black;7320047242915;31499-525;86.5;86.5;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;1
HERO 18KLM NARROW 4000K HTG_31504;307;7.3;4000;18118;498;18118;4000;4000;66;87;143;Black;Aluminium - Fagerhult - Black;7320046433833;31504;123;123;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 18KLM NARROW 4000K HTG_31504-461;307;7.3;4000;18118;498;18118;4000;4000;66;87;149;Black;Aluminium - Fagerhult - Black;7320046433857;31504-461;127.5;127.5;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 24KLM NARROW 4000K HTG_31507;307;7.3;4000;23878;498;23878;4000;4000;66;87;147;Black;Aluminium - Fagerhult - Black;7320046434069;31507;162;162;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;3;0
HERO 24KLM NARROW 4000K HTG_31507-461;307;7.3;4000;23878;498;23878;4000;4000;66;87;153;Black;Aluminium - Fagerhult - Black;7320046434083;31507-461;163;163;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;3;0
HERO 12KLM NARROW 4000K PMMA_31509;307;7.3;4000;12012;498;12012;4000;4000;66;87;147;Black;Aluminium - Fagerhult - Black;7320046433451;31509;82;82;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;0
HERO 12KLM NARROW 4000K PMMA_31509-461;307;7.3;4000;12012;498;12012;4000;4000;66;87;148;Black;Aluminium - Fagerhult - Black;7320046433499;31509-461;85;85;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;0
HERO 12KLM NARROW 4000K PMMA_31509-525;307;7.3;4000;12012;589;12012;4000;4000;65;102;146;Black;Aluminium - Fagerhult - Black;7320047242922;31509-525;86.5;86.5;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;1
HERO 18KLM NARROW 4000KPMMA_31514;307;7.3;4000;18064;498;18064;4000;4000;66;87;147;Black;Aluminium - Fagerhult - Black;7320046433864;31514;123;123;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 18KLM NARROW 4000KPMMA_31514-461;307;7.3;4000;18064;498;18064;4000;4000;66;87;148;Black;Aluminium - Fagerhult - Black;7320046433888;31514-461;127.5;127.5;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;0
HERO 18KLM NARROW 4000KPMMA_31514-525;307;7.3;4000;18064;589;18064;4000;4000;65;102;147;Black;Aluminium - Fagerhult - Black;7320047243028;31514-525;128.5;128.5;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;1
HERO 24KLM NARROW 4000K PMMA_31517;307;7.3;4000;23806;498;23806;4000;4000;66;87;147;Black;Aluminium - Fagerhult - Black;7320046434090;31517;162;162;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;3;0
HERO 24KLM NARROW 4000K PMMA_31517-461;307;7.3;4000;23806;498;23806;4000;4000;66;87;153;Black;Aluminium - Fagerhult - Black;7320046434120;31517-461;163;163;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;3;0
HERO 24KLM NARROW 4000K PMMA_31517-525;307;7.3;4000;23806;589;23806;4000;4000;65;102;151;Black;Aluminium - Fagerhult - Black;7320047243073;31517-525;165;165;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;3;1
HERO 24KLM NARROW 4000K HTG_31507-525;307;7.3;4000;23878;589;23878;4000;4000;65;102;152;Black;Aluminium - Fagerhult - Black;7320047161230;31507-525;165;165;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;3;1
HERO 12KLM NARROW 4000K HTG_31499-580;307;7.300;4000;12048;589;12048;4000;4000;65;102;146;Black;Aluminium - Fagerhult - Black;7316912758179;31499-580;86.5;86.5;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;1
HERO 18KLM NARROW 4000K HTG_31504-580;307;7.300;4000;18118;589;18118;4000;4000;65;102;147;Black;Aluminium - Fagerhult - Black;7316912758209;31504-580;128.5;128.5;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;1
HERO 24KLM NARROW 4000K HTG_31507-580;307;7.300;4000;23878;589;23878;4000;4000;65;102;152;Black;Aluminium - Fagerhult - Black;7316912758223;31507-580;165;165;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;3;1
HERO 12KLM NARROW 4000K PMMA_31509-580;307;7.300;4000;12012;589;12012;4000;4000;65;102;146;Black;Aluminium - Fagerhult - Black;7316912758193;31509-580;86.5;86.5;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;1;1
HERO 18KLM NARROW 4000KPMMA_31514-580;307;7.300;4000;18064;589;18064;4000;4000;65;102;147;Black;Aluminium - Fagerhult - Black;7316912758216;31514-580;128.5;128.5;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;2;1
HERO 24KLM NARROW 4000K PMMA_31517-580;307;7.300;4000;23806;589;23806;4000;4000;65;102;151;Black;Aluminium - Fagerhult - Black;7316912758230;31517-580;165;165;Hero Narrow Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1;3;1
