;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Louvre type##OTHER##;Luminaire type##OTHER##
NOTOR36 CEIL D 1200 DALI LL BETA 840_16086-20023;36;1.9;4000;1750;Aluminium - Fagerhult - Beta Opti Nano;1255;1750;4000;4000;20;36;128;White;Aluminium - Fagerhult - White;7320048598318;16086-20023;14.5;14.5;Notor 36 ceiling Beta Opti Nano;Keyhole slots permit individual or system surface-mounted installation.;Luminaire with Beta Opti Nano louvre for surface-mounted installation, individually or in a system.;min. 80;C;1;1;1
NOTOR36 CEIL D 2400 DALI LL BETA 840_16086-20024;36;3.2;4000;3500;Aluminium - Fagerhult - Beta Opti Nano;2507;3500;4000;4000;20;36;132;White;Aluminium - Fagerhult - White;7320048598349;16086-20024;28.5;28.5;Notor 36 ceiling Beta Opti Nano;Keyhole slots permit individual or system surface-mounted installation.;Luminaire with Beta Opti Nano louvre for surface-mounted installation, individually or in a system.;min. 80;C;1;2;1
NOTOR36 CEIL D 1200 DALI HL BETA 840_16086-20025;36;1.9;4000;2800;Aluminium - Fagerhult - Beta Opti Nano;1255;2800;4000;4000;20;36;135;White;Aluminium - Fagerhult - White;7320048598370;16086-20025;22.5;22.5;Notor 36 ceiling Beta Opti Nano;Keyhole slots permit individual or system surface-mounted installation.;Luminaire with Beta Opti Nano louvre for surface-mounted installation, individually or in a system.;min. 80;C;1;1;1
NOTOR36 CEIL D 2400 DALI HL BETA 840_16086-20026;36;3.2;4000;5600;Aluminium - Fagerhult - Beta Opti Nano;2507;5600;4000;4000;20;36;134;White;Aluminium - Fagerhult - White;7320048598400;16086-20026;44;44;Notor 36 ceiling Beta Opti Nano;Keyhole slots permit individual or system surface-mounted installation.;Luminaire with Beta Opti Nano louvre for surface-mounted installation, individually or in a system.;min. 80;C;1;2;1
NOTOR36 CEIL D 1200 DALI LL BETA 840_16086-20063;36;1.9;4000;1750;Aluminium - Fagerhult - Beta Opti Nano;1268;1750;4000;4000;20;36;128;White;Aluminium - Fagerhult - White;7320048855312;16086-20063;14.5;14.5;Notor 36 ceiling Beta Opti Nano;Keyhole slots permit individual or system surface-mounted installation.;Luminaire with Beta Opti Nano louvre for surface-mounted installation, individually or in a system.;min. 80;C;1;1;3
NOTOR36 CEIL D 2400 DALI LL BETA 840_16086-20065;36;3.2;4000;3500;Aluminium - Fagerhult - Beta Opti Nano;2520;3500;4000;4000;20;36;136;White;Aluminium - Fagerhult - White;7320048855398;16086-20065;27;27;Notor 36 ceiling Beta Opti Nano;Keyhole slots permit individual or system surface-mounted installation.;Luminaire with Beta Opti Nano louvre for surface-mounted installation, individually or in a system.;min. 80;C;1;2;3
NOTOR36 CEIL D 1200 DALI LL BETA 840_16086-20066;36;1.9;4000;1750;Aluminium - Fagerhult - Beta Opti Nano;1254;1750;4000;4000;20;36;128;White;Aluminium - Fagerhult - White;7320048855428;16086-20066;14.5;14.5;Notor 36 ceiling Beta Opti Nano;Keyhole slots permit individual or system surface-mounted installation.;Luminaire with Beta Opti Nano louvre for surface-mounted installation, individually or in a system.;min. 80;C;1;1;2
NOTOR36 CEIL D 2400 DALI LL BETA 840_16086-20068;36;3.2;4000;3500;Aluminium - Fagerhult - Beta Opti Nano;2506;3500;4000;4000;20;36;136;White;Aluminium - Fagerhult - White;7320048855480;16086-20068;27;27;Notor 36 ceiling Beta Opti Nano;Keyhole slots permit individual or system surface-mounted installation.;Luminaire with Beta Opti Nano louvre for surface-mounted installation, individually or in a system.;min. 80;C;1;2;2
