;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
MULTILUME FUNCTION BASIC DALI 1800 110X80 3000K WHITE_44092-510;110;5.2;3000;9021;Aluminium - Fagerhult - Beta Opti;1924;9021;3000;3000;20;80;141;White;Steel - Fagerhult - White;7316911794215;44092-510;64;64;Multilume Function Basic;The luminaire is  designed for mounting in functional ceiling 110-80, 1800/2000 module.;Illuminate the store in a comfortable way with reduced glare and decreased energy consumption with Multilume Function Basic. This luminaire is designed to easily install in a function ceiling.;min. 80;C;1
MULTILUME FUNCTION BASIC DALI 1800 110X80 3000K WHITE_44092-512;110;5.2;3000;9021;Aluminium - Fagerhult - Beta Opti;1924;9021;3000;3000;20;80;141;White;Steel - Fagerhult - White;7316911794239;44092-512;64;64;Multilume Function Basic;The luminaire is  designed for mounting in functional ceiling 110-80, 1800/2000 module.;Illuminate the store in a comfortable way with reduced glare and decreased energy consumption with Multilume Function Basic. This luminaire is designed to easily install in a function ceiling.;min. 80;C;1
MULTILUME FUNCTION BASIC 1800 110X80 3000K WHITE_44091-3;110;5.2;3000;9021;Aluminium - Fagerhult - Beta Opti;1724;9021;3000;3000;20;80;141;White;Steel - Fagerhult - White;7316911794192;44091-3;64;64;Multilume Function Basic;The luminaire is  designed for mounting in functional ceiling 110-80, 1800/2000 module.;Illuminate the store in a comfortable way with reduced glare and decreased energy consumption with Multilume Function Basic. This luminaire is designed to easily install in a function ceiling.;min. 80;C;1
MULTILUME FUNCTION BASIC 1800 110X80 3000K WHITE_44091-303;110;5.2;3000;9021;Aluminium - Fagerhult - Beta Opti;1724;9021;3000;3000;20;80;141;White;Steel - Fagerhult - White;7316911794208;44091-303;64;64;Multilume Function Basic;The luminaire is  designed for mounting in functional ceiling 110-80, 1800/2000 module.;Illuminate the store in a comfortable way with reduced glare and decreased energy consumption with Multilume Function Basic. This luminaire is designed to easily install in a function ceiling.;min. 80;C;1
MULTILUME FUNCTION BASIC 2000 110X80 3500K WHITE_44090-3;110;5.7;3500;9658;Aluminium - Fagerhult - Beta Opti;1924;9658;3500;3500;20;80;140;White;Steel - Fagerhult - White;7316911794161;44090-3;69;69;Multilume Function Basic;The luminaire is  designed for mounting in functional ceiling 110-80, 1800/2000 module.;Illuminate the store in a comfortable way with reduced glare and decreased energy consumption with Multilume Function Basic. This luminaire is designed to easily install in a function ceiling.;min. 80;C;1
MULTILUME FUNCTION BASIC 2000 110X80 3500K WHITE_44090-303;110;5.7;3500;9658;Aluminium - Fagerhult - Beta Opti;1924;9658;3500;3500;20;80;140;White;Steel - Fagerhult - White;7316911794178;44090-303;69;69;Multilume Function Basic;The luminaire is  designed for mounting in functional ceiling 110-80, 1800/2000 module.;Illuminate the store in a comfortable way with reduced glare and decreased energy consumption with Multilume Function Basic. This luminaire is designed to easily install in a function ceiling.;min. 80;C;1
