;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;End Cap 1##OTHER##;End Cap 2##OTHER##;Organic##OTHER##;Continuous##OTHER##
NOTOR65 ASYM RIGHT SURF PEND 1200 HL 840 ALU CONT_13619-402;65;3;4000;3772;PMMA - Fagerhult - Frosted acrylic;1250;3772;4000;4000;20;65;136;Anodised;Aluminium - Fagerhult - Anodised;7320048883179;13619-402;29;29;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;0;0;0;1
NOTOR65 ASYM RIGHT SURF PEND 1200 LL 830 BLACK CONT_13624-402;65;3;3000;1494;PMMA - Fagerhult - Frosted acrylic;1250;1494;3000;3000;20;65;130;Black;Aluminium - Fagerhult - Black;7320048883278;13624-402;12.5;12.5;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;0;0;0;1
NOTOR65 ASYM LEFT SURF PEND 1000 LL 830 WHT CONT_13628-402;65;2.5;3000;1234;PMMA - Fagerhult - Frosted acrylic;1025;1234;3000;3000;20;65;127;White;Aluminium - Fagerhult - White;7320048883353;13628-402;10.5;10.5;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;0;0;0;1
NOTOR65 ASYM LEFT SURF PEND 2000 LL 830 WHT START/SINGLE_13632-402;65;4.6;3000;2469;PMMA - Fagerhult - Frosted acrylic;2043;2469;3000;3000;20;65;132;White;Aluminium - Fagerhult - White;7320048883438;13632-402;19.5;19.5;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;1;1;0;0
NOTOR 65 SURF/PEND ASYM LEFT 2000 LL 830_13632-533;65;4.8;3000;2469;PMMA - Fagerhult - Frosted acrylic;2133;2469;3000;3000;20;65;132;White;Aluminium - Fagerhult - White;7320048883452;13632-533;20;20;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;1;1;1;0
NOTOR65 ASYM LEFT SURF PEND 1200 HL 830 WHT START/SINGLE_13585-402;65;3.1;3000;3667;PMMA - Fagerhult - Frosted acrylic;1256;3667;3000;3000;20;65;132;White;Aluminium - Fagerhult - White;7320048882493;13585-402;29;29;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;1;1;0;0
NOTOR65 ASYM LEFT SURF PEND 1200 HL 840 WHT START/SINGLE_13587-402;65;3.1;4000;3772;PMMA - Fagerhult - Frosted acrylic;1256;3772;4000;4000;20;65;136;White;Aluminium - Fagerhult - White;7320048882530;13587-402;29;29;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;1;1;0;0
NOTOR65 ASYM LEFT SURF PEND 1200 LL 830 BLACK START/SINGLE_13588-402;65;3.1;3000;1494;PMMA - Fagerhult - Frosted acrylic;1256;1494;3000;3000;20;65;130;Black;Aluminium - Fagerhult - Black;7320048882554;13588-402;12.5;12.5;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;1;1;0;0
NOTOR65 ASYM LEFT SURF PEND 2000 LL 830 WHT CONT_13644-402;65;4.7;3000;2469;PMMA - Fagerhult - Frosted acrylic;2037;2469;3000;3000;20;65;132;White;Aluminium - Fagerhult - White;7320048883711;13644-402;19.5;19.5;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;0;0;0;1
NOTOR 65 SURF/PEND ASYM RIGHT 2000 HL 830_13669-20004;65;4.8;3000;6059;PMMA - Fagerhult - Frosted acrylic;2043;6059;3000;3000;20;65;138;Alugrey;Aluminium - Fagerhult - Alugrey;7316911519801;13669-20004;46;46;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;1;1;0;0
NOTOR 65 SURF/PEND ASYM RIGHT 1200 LL 830_13669-20005;65;3;3000;1494;PMMA - Fagerhult - Frosted acrylic;1256;1494;3000;3000;20;65;130;Alugrey;Aluminium - Fagerhult - Alugrey;7316911519832;13669-20005;12.5;12.5;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;1;1;0;0
NOTOR 65 SURF/PEND ASYM RIGHT 2000 LL 840_13669-20006;65;4.5;4000;2540;PMMA - Fagerhult - Frosted acrylic;2043;2540;4000;4000;20;65;136;Black;Aluminium - Fagerhult - Black;7316911519863;13669-20006;19.5;19.5;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;1;1;0;0
NOTOR 65 SURF/PEND ASYM LEFT 2000 LL 830_13669-20007;65;4.7;3000;2469;PMMA - Fagerhult - Frosted acrylic;2133;2469;3000;3000;20;65;132;White;Aluminium - Fagerhult - White;7316911519894;13669-20007;20;20;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;1;1;0;0
NOTOR 65 SURF/PEND ASYM LEFT 1200 HL 830_13669-20008;65;3;3000;3667;PMMA - Fagerhult - Frosted acrylic;1256;3667;3000;3000;20;65;132;White;Aluminium - Fagerhult - White;7316911519924;13669-20008;29;29;Notor 65 Asymmetrical;"Single or continuous installation in wire suspension or surface mounted. For wire suspension mounting, a wire bracket is required for flexible c/c; see accessories. Can also be mounted on walls or bookcases with bracket; see accessories.";Suspended or ceiling mounted with asymmetric light and Opal louvre shutters. Single or continuous installation. Can also be mounted on wall or bookcase with bracket.;min. 80;C;3;1;1;1;0