;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
EXCIS LED ASYMMETRIC 20300LM 3000K_18448-402;324;9.000;3000;19799;Plastic - Fagerhult - Optical line prism;1156;19799;3000;3000;20;94;150;White;Aluminium - Fagerhult - White;7320046288808;18448-402;140;140;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;C;1
EXCIS LED WIDE 20300LM 3000K_18445-402;324;9.000;3000;19880;Plastic - Fagerhult - Optical line prism;1156;19880;3000;3000;20;94;151;White;Aluminium - Fagerhult - White;7320046288686;18445-402;140;140;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;C;1
EXCIS LED ASYMMETRIC 20300LM 4000K_18457-402;324;9.000;4000;20863;Plastic - Fagerhult - Optical line prism;1156;20863;4000;4000;20;94;158;White;Aluminium - Fagerhult - White;7320046289164;18457-402;140;140;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;B;1
EXCIS LED WIDE 12000LM 3000K_18444-402;324;9.000;3000;11630;Plastic - Fagerhult - Optical line prism;1156;11630;3000;3000;20;94;159;White;Aluminium - Fagerhult - White;7320046288648;18444-402;77.5;77.5;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;C;1
EXCIS LED WIDE 20300LM 4000K_18454-402;324;9.000;4000;20282;Plastic - Fagerhult - Optical line prism;1156;20282;4000;4000;20;94;162;White;Aluminium - Fagerhult - White;7320046289041;18454-402;140;140;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;C;1
EXCIS LED MEDIUM 6000LM 4000K_18449-402;324;9.000;4000;6621;Plastic - Fagerhult - Optical line prism;1156;6621;4000;4000;20;94;166;White;Aluminium - Fagerhult - White;7320046288846;18449-402;43;43;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;B;1
EXCIS LED MEDIUM 20300LM 3000K_18442-402;324;9.000;3000;20142;Plastic - Fagerhult - Optical line prism;1156;20142;3000;3000;20;94;153;White;Aluminium - Fagerhult - White;7320046288563;18442-402;140;140;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;C;1
EXCIS LED MEDIUM 20300LM 4000K_18451-402;324;9.000;4000;20549;Plastic - Fagerhult - Optical line prism;1156;20549;4000;4000;20;94;156;White;Aluminium - Fagerhult - White;7320046288921;18451-402;140;140;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;B;1
EXCIS LED MEDIUM 12000LM 3000K_18441-402;324;9.000;3000;11182;Plastic - Fagerhult - Optical line prism;1156;11182;3000;3000;20;94;153;White;Aluminium - Fagerhult - White;7320046288525;18441-402;77.5;77.5;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;C;1
EXCIS LED WIDE 6000LM 4000K_18452-402;324;9.000;4000;6535;Plastic - Fagerhult - Optical line prism;1156;6535;4000;4000;20;94;163;White;Aluminium - Fagerhult - White;7320046288969;18452-402;43;43;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;B;1
EXCIS LED ASYMMETRIC 12000LM 4000K_18456-402;324;9.000;4000;11583;Plastic - Fagerhult - Optical line prism;1156;11583;4000;4000;20;94;159;White;Aluminium - Fagerhult - White;7320046289126;18456-402;77.5;77.5;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;B;1
EXCIS LED WIDE 12000LM 4000K_18453-402;324;9.000;4000;11630;Plastic - Fagerhult - Optical line prism;1156;11630;4000;4000;20;94;159;White;Aluminium - Fagerhult - White;7320046289003;18453-402;77.5;77.5;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;B;1
EXCIS LED ASYMMETRIC 12000LM 3000K_18447-402;324;9.000;4000;10992;Plastic - Fagerhult - Optical line prism;1156;10992;4000;4000;20;94;151;White;Aluminium - Fagerhult - White;7320046288761;18447-402;77.5;77.5;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;B;1
EXCIS LED WIDE 6000LM 3000K_18443-402;324;9.000;3000;6201;Plastic - Fagerhult - Optical line prism;1156;6201;3000;3000;20;94;155;White;Aluminium - Fagerhult - White;7320046288600;18443-402;43;43;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;C;1
EXCIS LED ASYMMETRIC 6000LM 3000K_18446-402;324;9.000;3000;6176;Plastic - Fagerhult - Optical line prism;1156;6176;3000;3000;20;94;154;White;Aluminium - Fagerhult - White;7320046288723;18446-402;43;43;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;C;1
EXCIS LED ASYMMETRIC 6000LM 4000K_18455-402;324;9.000;4000;6508;Plastic - Fagerhult - Optical line prism;1156;6508;4000;4000;20;94;163;White;Aluminium - Fagerhult - White;7320046289089;18455-402;43;43;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;B;1
EXCIS LED MEDIUM 6000LM 3000K_18440-402;324;9.000;3000;6283;Plastic - Fagerhult - Optical line prism;1156;6283;3000;3000;20;94;157;White;Aluminium - Fagerhult - White;7320046288488;18440-402;43;43;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;C;1
EXCIS LED MEDIUM 12000LM 4000K_18450-402;324;9.000;4000;11783;Plastic - Fagerhult - Optical line prism;1156;11783;4000;4000;20;94;161;White;Aluminium - Fagerhult - White;7320046288884;18450-402;77.5;77.5;Excis;"Luminaire for surface-mounted ceiling installation, on cable with cable brackets, tube with tube bracket or adjustable ceiling bracket. See brackets under Accessories.
For detailed information, see the installation instructions.";Excis is specially developed for sports halls. The luminaire is certified for ball impact resistance and has high luminous fluxes and several light distribution options. Good lighting makes it easy to follow the game.;min. 80;B;1
