;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Type##OTHER##
SENTRA 3-PHASE ADAPTER OPAL WIDE 1200 STD HL 830_45100-20004;3.7;3000;7095;PMMA - Fagerhult - Opal;1262;20;96;139;White;Aluminium - Fagerhult - White;7316910861451;45100-20004;51;Sentra;On rail Lighting Track Pro (on/off) or Control Track (DALI).;A rail-mounted linear luminaire with a softly rounded inner profile and 3 different light distribution patterns that meet the lighting requirements of larger stores, such as hypermarkets and department stores. The Sentra is available in 2 lengths, 1200 mm and 1800 mm.;min. 80;C;1;1
SENTRA 3-PHASE ADAPTER ASYM 1200 STD HL 830_45100-20008;3.7;3000;7105;Acrylic - Fagerhult - Lens;1213;20;96;140;White;Aluminium - Fagerhult - White;7316910861482;45100-20008;51;Sentra;On rail Lighting Track Pro (on/off) or Control Track (DALI).;A rail-mounted linear luminaire with a softly rounded inner profile and 3 different light distribution patterns that meet the lighting requirements of larger stores, such as hypermarkets and department stores. The Sentra is available in 2 lengths, 1200 mm and 1800 mm.;min. 80;C;1;2
SENTRA 3-PHASE ADAPTER DOUBLE ASYM 1200 STD HL 830_45100-20009;3.7;3000;7358;Acrylic - Fagerhult - Lens;1213;20;96;145;White;Aluminium - Fagerhult - White;7316910861512;45100-20009;51;Sentra;On rail Lighting Track Pro (on/off) or Control Track (DALI).;A rail-mounted linear luminaire with a softly rounded inner profile and 3 different light distribution patterns that meet the lighting requirements of larger stores, such as hypermarkets and department stores. The Sentra is available in 2 lengths, 1200 mm and 1800 mm.;min. 80;C;1;3
SENTRA 3-PHASE ADAPTER OPAL WIDE 1800 STD HL 830_45100-20003;5.1;3000;10051;PMMA - Fagerhult - Opal;1786;20;96;144;White;Aluminium - Fagerhult - White;7316910861543;45100-20003;70;Sentra;On rail Lighting Track Pro (on/off) or Control Track (DALI).;A rail-mounted linear luminaire with a softly rounded inner profile and 3 different light distribution patterns that meet the lighting requirements of larger stores, such as hypermarkets and department stores. The Sentra is available in 2 lengths, 1200 mm and 1800 mm.;min. 80;C;1;1
SENTRA 3-PHASE ADAPTER ASYM 1800 STD HL 830_45100-20010;5.2;3000;10658;Acrylic - Fagerhult - Lens;1814;20;96;146;White;Aluminium - Fagerhult - White;7316910861574;45100-20010;73;Sentra;On rail Lighting Track Pro (on/off) or Control Track (DALI).;A rail-mounted linear luminaire with a softly rounded inner profile and 3 different light distribution patterns that meet the lighting requirements of larger stores, such as hypermarkets and department stores. The Sentra is available in 2 lengths, 1200 mm and 1800 mm.;min. 80;C;1;2
SENTRA 3-PHASE ADAPTER DOUBLE ASYM 1800 STD HL 830_45100-20002;5.2;3000;11037;Acrylic - Fagerhult - Lens;1814;20;96;151;White;Aluminium - Fagerhult - White;7316910723667;45100-20002;73;Sentra;On rail Lighting Track Pro (on/off) or Control Track (DALI).;A rail-mounted linear luminaire with a softly rounded inner profile and 3 different light distribution patterns that meet the lighting requirements of larger stores, such as hypermarkets and department stores. The Sentra is available in 2 lengths, 1200 mm and 1800 mm.;min. 80;C;1;3
